17:35:19.676 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:35:20.133 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:35:20.135 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:35:20.140 -> [PIMA] pima_read_cycle: attempt 1 -> fail
17:35:20.143 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:35:21.609 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:35:28.305 -> [KEYS] Loaded from flash
17:35:28.308 -> DEVEUI:ac1f0926002f0003
17:35:28.311 -> APPKEY:f2839693c180a9df89412e3098ba5a43
17:35:28.317 -> MODEL:ST-EAM-01B
17:35:28.323 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
17:35:28.381 -> 5s052:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
17:35:28.390 -> [LORA] Starting join (OTAA)
17:35:28.393 -> 5s059:TX on freq 915400000 Hz at DR 2
17:35:28.699 -> 5s432:MAC txDone
17:35:33.645 -> 10s409:RX_1 on freq 923900000 Hz at DR 10
17:35:33.699 -> 10s458:IRQ_RX_TX_TIMEOUT
17:35:33.704 -> 10s458:MAC rxTimeOut
17:35:34.666 -> 11s420:RX_2 on freq 923300000 Hz at DR 8
17:35:34.721 -> 11s487:IRQ_RX_TX_TIMEOUT
17:35:34.724 -> 11s487:MAC rxTimeOut
17:35:34.779 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
17:35:34.784 -> 
17:35:34.790 -> [LORA] JOIN FAILED (status=-1) count=1
17:35:34.795 -> [LORA] Rejoin scheduled
17:35:44.738 -> 21s493:TX on freq 917200000 Hz at DR 2
17:35:44.741 -> [LORA] Rejoin busy -> retry in 5000 ms
17:35:45.102 -> 21s866:MAC txDone
17:35:49.749 -> [LORA] Rejoin busy -> retry in 5000 ms
17:35:50.109 -> 26s843:RX_1 on freq 924500000 Hz at DR 10
17:35:50.215 -> 26s982:MAC rxDone
17:35:50.270 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
17:35:50.274 -> 27s003:RX_C on freq 923300000 Hz at DR 8
17:35:50.277 -> [LORA] Switch to Class C done
17:35:50.283 -> 
17:35:50.292 -> [LORA] JOINED (OTAA)
17:35:50.300 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
17:35:50.308 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
17:35:50.315 -> ###### NwkSKey:     42:43:58:88:82:10:64:41:A9:BD:68:E8:E0:96:E0:36
17:35:50.318 -> ###### AppSKey:     A2:CA:21:BA:2C:E3:9D:4F:95:2C:9C:B9:C1:78:DC:0C
17:35:58.244 -> [PIMA] B1 warmup uplink
17:35:58.250 -> 
17:35:58.252 -> [PIMA] Uplink routine
17:35:58.262 -> [BOOT] Sending initial warmup byte (B1)
17:35:58.270 -> 35s004:TX on freq 917000000 Hz at DR 2
17:35:58.533 -> 35s295:MAC txDone
17:35:58.537 -> 35s296:RX_C on freq 923300000 Hz at DR 8
17:36:03.493 -> 40s266:RX_1 on freq 923900000 Hz at DR 10
17:36:03.652 -> 40s380:MAC rxDone
17:36:03.657 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=9
17:36:03.664 -> [RX] port=0 size=0
17:36:03.674 -> 40s387:RX_C on freq 923300000 Hz at DR 8
17:36:06.251 -> [PIMA] First read after boot
17:36:06.262 -> [PIMA] Changing to OTAA_PERIOD mode
17:36:06.268 -> [LORA] Phase offset applied once: 3244 ms (base=900000 ms)
17:36:06.274 -> 
17:36:06.277 -> [PIMA] Uplink routine
17:36:06.281 -> [PIMA] pima_read_cycle: start (burstMax=60)
17:36:06.287 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:36:07.709 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:09.179 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:10.650 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:12.123 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:13.592 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:14.055 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:36:14.061 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:36:14.070 -> [PIMA] pima_read_cycle: attempt 1 -> fail
17:36:14.083 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:36:15.506 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:16.979 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:18.449 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:19.917 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:21.391 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:36:21.852 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:36:21.914 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:36:21.924 -> [PIMA] pima_read_cycle: attempt 2 -> fail
17:36:21.935 -> [PIMA] pima_read_cycle: overall timeout reached
17:36:21.944 -> [PIMA] pima_read_cycle: no packet captured
17:36:21.953 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
17:36:21.963 -> 58s629:TX on freq 916800000 Hz at DR 5
17:36:22.022 -> 58s773:MAC txDone
17:36:22.030 -> 58s774:RX_C on freq 923300000 Hz at DR 8
17:36:26.985 -> 63s741:RX_1 on freq 923300000 Hz at DR 13
17:36:27.042 -> 63s787:MAC rxDone
17:36:27.048 -> 63s788:IRQ_CRC_ERROR
17:36:27.059 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=8
17:36:27.072 -> 63s793:RX_C on freq 923300000 Hz at DR 8
17:39:06.109 -> [KEYS] Loaded from flash
17:39:06.114 -> DEVEUI:ac1f0926002f0003
17:39:06.119 -> APPKEY:f2839693c180a9df89412e3098ba5a43
17:39:06.122 -> MODEL:ST-EAM-01B
17:39:06.126 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
17:39:06.182 -> 5s052:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
17:39:06.195 -> [LORA] Starting join (OTAA)
17:39:06.200 -> 5s059:TX on freq 915200000 Hz at DR 2
17:39:06.511 -> 5s432:MAC txDone
17:39:11.460 -> 10s409:RX_1 on freq 923300000 Hz at DR 10
17:39:11.512 -> 10s458:IRQ_RX_TX_TIMEOUT
17:39:11.517 -> 10s458:MAC rxTimeOut
17:39:12.483 -> 11s420:RX_2 on freq 923300000 Hz at DR 8
17:39:12.537 -> 11s486:IRQ_RX_TX_TIMEOUT
17:39:12.545 -> 11s487:MAC rxTimeOut
17:39:12.556 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
17:39:12.568 -> 
17:39:12.577 -> [LORA] JOIN FAILED (status=-1) count=1
17:39:12.583 -> [LORA] Rejoin scheduled
17:39:22.529 -> 21s493:TX on freq 917600000 Hz at DR 2
17:39:22.541 -> [LORA] Rejoin busy -> retry in 5000 ms
17:39:22.901 -> 21s866:MAC txDone
17:39:27.544 -> [LORA] Rejoin busy -> retry in 5000 ms
17:39:27.901 -> 26s843:RX_1 on freq 925700000 Hz at DR 10
17:39:28.054 -> 26s982:MAC rxDone
17:39:28.059 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
17:39:28.063 -> 27s003:RX_C on freq 923300000 Hz at DR 8
17:39:28.070 -> [LORA] Switch to Class C done
17:39:28.078 -> 
17:39:28.084 -> [LORA] JOINED (OTAA)
17:39:28.091 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
17:39:28.098 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
17:39:28.150 -> ###### NwkSKey:     77:44:F9:9A:69:1F:60:19:A1:D9:ED:FF:77:3D:E3:50
17:39:28.154 -> ###### AppSKey:     AB:6F:0B:D3:CF:DE:AE:E8:69:E8:E8:9D:55:8C:F3:CD
17:39:36.032 -> [PIMA] B1 warmup uplink
17:39:36.042 -> 
17:39:36.109 -> [PIMA] Uplink routine
17:39:36.119 -> [BOOT] Sending initial warmup byte (B1)
17:39:36.136 -> 35s004:TX on freq 917000000 Hz at DR 2
17:39:36.352 -> 35s295:MAC txDone
17:39:36.367 -> 35s296:RX_C on freq 923300000 Hz at DR 8
17:39:41.322 -> 40s266:RX_1 on freq 923900000 Hz at DR 10
17:39:41.438 -> 40s380:MAC rxDone
17:39:41.453 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=9
17:39:41.472 -> [RX] port=0 size=0
17:39:41.485 -> 40s387:RX_C on freq 923300000 Hz at DR 8
17:39:44.038 -> [PIMA] First read after boot
17:39:44.042 -> [PIMA] Changing to OTAA_PERIOD mode
17:39:44.076 -> [LORA] Phase offset applied once: 3244 ms (base=900000 ms)
17:39:44.102 -> 
17:39:44.175 -> 
17:39:44.188 -> [PIMA] Uplink routine
17:39:44.220 -> [PIMA] pima_read_cycle: start (burstMax=60)
17:39:44.241 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:39:45.528 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:47.007 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:48.437 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:49.919 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:51.357 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:51.884 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:39:51.899 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:39:51.927 -> [PIMA] pima_read_cycle: attempt 1 -> fail
17:39:51.942 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:39:53.328 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:54.805 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:56.286 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:57.712 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:59.191 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:39:59.660 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:39:59.678 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:39:59.757 -> [PIMA] pima_read_cycle: attempt 2 -> fail
17:39:59.770 -> [PIMA] pima_read_cycle: overall timeout reached
17:39:59.794 -> [PIMA] pima_read_cycle: no packet captured
17:39:59.816 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
17:39:59.840 -> 58s629:TX on freq 916800000 Hz at DR 5
17:39:59.916 -> 58s773:MAC txDone
17:39:59.935 -> 58s774:RX_C on freq 923300000 Hz at DR 8
17:40:04.802 -> 63s741:RX_1 on freq 923300000 Hz at DR 13
17:40:04.872 -> 63s787:MAC rxDone
17:40:04.893 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=8
17:40:04.927 -> [RX] port=0 size=0
17:40:04.963 -> 63s794:RX_C on freq 923300000 Hz at DR 8
17:43:29.457 -> 268s460:MAC rxDone
17:43:29.470 -> [RX] port=1 size=1
17:43:29.494 -> [RX] payload: 05 
17:43:29.568 -> [CMD] Simple command received: cmd=0x05, size=1
17:43:29.575 -> [CMD][DEBUG] Entering debug mode
17:43:29.587 -> [DEBUG] Debug mode ON (Tx=35000 ms, duration=300000 ms)
17:43:29.610 -> [CMD] ACK cmd=0x05 status=OK
17:43:29.622 -> [CMD] SendResponse: size=1
17:43:29.634 -> 268s469:TX on freq 918200000 Hz at DR 5
17:43:29.655 -> 268s523:MAC txDone
17:43:29.674 -> 268s523:RX_C on freq 923300000 Hz at DR 8
17:43:34.489 -> 273s491:RX_1 on freq 927500000 Hz at DR 13
17:43:34.548 -> 273s537:MAC rxDone
17:43:34.554 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=3, Channel=15
17:43:34.563 -> [RX] port=0 size=0
17:43:34.568 -> 273s543:RX_C on freq 923300000 Hz at DR 8
17:43:39.674 -> 278s676:MAC rxDone
17:43:39.681 -> 278s682:RX_C on freq 923300000 Hz at DR 8
17:44:02.391 -> 301s374:MAC rxDone
17:44:02.404 -> 301s379:RX_C on freq 923300000 Hz at DR 8
17:44:04.486 -> [LORA] Next period armed: 35000 ms (phaseOnce=3244)
17:44:04.503 -> 
17:44:04.524 -> [PIMA] Uplink routine
17:44:04.556 -> [PIMA] pima_read_cycle: start (burstMax=60)
17:44:04.564 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:44:05.942 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:07.419 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:08.848 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:10.328 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:11.806 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:12.273 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:44:12.288 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:44:12.309 -> [PIMA] pima_read_cycle: attempt 1 -> fail
17:44:12.376 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:44:13.759 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:15.227 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:16.695 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:18.164 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:19.632 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:44:20.094 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:44:20.100 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:44:20.108 -> [PIMA] pima_read_cycle: attempt 2 -> fail
17:44:20.115 -> [PIMA] pima_read_cycle: overall timeout reached
17:44:20.125 -> [PIMA] pima_read_cycle: no packet captured
17:44:20.135 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
17:44:20.197 -> 319s090:TX on freq 917200000 Hz at DR 5
17:44:20.255 -> 319s229:MAC txDone
17:44:20.260 -> 319s230:RX_C on freq 923300000 Hz at DR 8
17:44:30.928 -> [KEYS] Loaded from flash
17:44:30.984 -> DEVEUI:ac1f0926002f0003
17:44:30.988 -> APPKEY:f2839693c180a9df89412e3098ba5a43
17:44:30.996 -> MODEL:ST-EAM-01B
17:44:31.003 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
17:44:31.008 -> 5s052:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
17:44:31.023 -> [LORA] Starting join (OTAA)
17:44:31.027 -> 5s059:TX on freq 915800000 Hz at DR 2
17:44:31.335 -> 5s432:MAC txDone
17:44:36.338 -> 10s409:RX_1 on freq 925100000 Hz at DR 10
17:44:36.341 -> 10s458:IRQ_RX_TX_TIMEOUT
17:44:36.400 -> 10s458:MAC rxTimeOut
17:44:37.315 -> 11s420:RX_2 on freq 923300000 Hz at DR 8
17:44:37.372 -> 11s486:IRQ_RX_TX_TIMEOUT
17:44:37.377 -> 11s487:MAC rxTimeOut
17:44:37.433 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
17:44:37.443 -> 
17:44:37.456 -> [LORA] JOIN FAILED (status=-1) count=1
17:44:37.467 -> [LORA] Rejoin scheduled
17:44:47.421 -> 21s493:TX on freq 917600000 Hz at DR 2
17:44:47.428 -> [LORA] Rejoin busy -> retry in 5000 ms
17:44:47.788 -> 21s866:MAC txDone
17:44:52.388 -> [LORA] Rejoin busy -> retry in 5000 ms
17:44:52.753 -> 26s843:RX_1 on freq 925700000 Hz at DR 10
17:44:52.866 -> 26s982:MAC rxDone
17:44:52.926 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
17:44:52.928 -> 27s003:RX_C on freq 923300000 Hz at DR 8
17:44:52.946 -> [LORA] Switch to Class C done
17:44:52.963 -> 
17:44:52.977 -> [LORA] JOINED (OTAA)
17:44:52.992 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
17:44:53.009 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
17:44:53.027 -> ###### NwkSKey:     DF:6F:FD:63:AF:49:E9:AD:BE:66:7F:D3:A5:14:CD:E3
17:44:53.046 -> ###### AppSKey:     87:59:CD:0F:9F:EC:70:00:0D:83:62:20:08:F7:27:C6
17:45:00.418 -> 34s513:MAC rxDone
17:45:00.431 -> 34s519:RX_C on freq 923300000 Hz at DR 8
17:45:00.886 -> [PIMA] B1 warmup uplink
17:45:00.897 -> 
17:45:00.919 -> [PIMA] Uplink routine
17:45:00.930 -> [BOOT] Sending initial warmup byte (B1)
17:45:01.007 -> 35s004:TX on freq 917200000 Hz at DR 2
17:45:01.183 -> 35s295:MAC txDone
17:45:01.198 -> 35s296:RX_C on freq 923300000 Hz at DR 8
17:45:06.167 -> 40s266:RX_1 on freq 924500000 Hz at DR 10
17:45:06.286 -> 40s380:MAC rxDone
17:45:06.305 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=10
17:45:06.312 -> [RX] port=0 size=0
17:45:06.326 -> 40s387:RX_C on freq 923300000 Hz at DR 8
17:45:08.919 -> [PIMA] First read after boot
17:45:08.935 -> [PIMA] Changing to OTAA_PERIOD mode
17:45:08.958 -> [LORA] Phase offset applied once: 3244 ms (base=900000 ms)
17:45:08.975 -> 
17:45:08.995 -> [PIMA] Uplink routine
17:45:09.016 -> [PIMA] pima_read_cycle: start (burstMax=60)
17:45:09.036 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:45:10.366 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:11.841 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:12.760 -> 46s839:MAC rxDone
17:45:13.275 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:14.034 -> 48s153:MAC rxDone
17:45:14.757 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:16.230 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:16.701 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:45:16.716 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:45:16.739 -> [PIMA] pima_read_cycle: attempt 1 -> fail
17:45:16.814 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
17:45:18.193 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:19.670 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:21.093 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:21.759 -> 55s841:MAC rxDone
17:45:22.583 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:22.944 -> 57s029:MAC rxDone
17:45:23.969 -> 58s083:MAC rxDone
17:45:24.028 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
17:45:24.549 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
17:45:24.565 -> [PIMA] Base frame 0x02 search timeout (no base found)
17:45:24.576 -> [PIMA] pima_read_cycle: attempt 2 -> fail
17:45:24.601 -> [PIMA] pima_read_cycle: overall timeout reached
17:45:24.622 -> [PIMA] pima_read_cycle: no packet captured
17:45:24.643 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
17:45:24.663 -> 58s629:TX on freq 917800000 Hz at DR 5
17:45:24.680 -> [LORA] OnTxData: status=1, DR=5, UplinkCounter=2, Channel=13
17:45:24.700 -> 58s640:RX_C on freq 923300000 Hz at DR 8
17:45:28.346 -> 62s456:MAC rxDone
17:45:28.364 -> 62s462:RX_C on freq 923300000 Hz at DR 8
17:45:28.538 -> 62s634:MAC txTimeOut
17:45:33.703 -> 67s829:MAC rxDone
17:45:33.771 -> 67s835:RX_C on freq 923300000 Hz at DR 8
17:45:46.847 -> 80s971:MAC rxDone
17:45:46.907 -> 80s977:RX_C on freq 923300000 Hz at DR 8
17:45:52.674 -> 86s776:MAC rxDone
17:45:52.685 -> 86s782:RX_C on freq 923300000 Hz at DR 8
17:45:55.635 -> 89s753:MAC rxDone
17:45:55.646 -> 89s759:RX_C on freq 923300000 Hz at DR 8
17:46:41.374 -> 135s479:MAC rxDone
17:46:41.381 -> 135s486:RX_C on freq 923300000 Hz at DR 8
17:48:57.206 -> 271s341:MAC rxDone
17:48:57.219 -> 271s347:RX_C on freq 923300000 Hz at DR 8
17:49:31.604 -> 305s762:MAC rxDone
17:49:31.609 -> [RX] port=1 size=1
17:49:31.620 -> [RX] payload: 00 
17:49:31.691 -> [CMD] Simple command received: cmd=0x00, size=1
17:49:31.697 -> [CMD] Unknown simple command: 0x00
17:49:31.710 -> 305s770:RX_C on freq 923300000 Hz at DR 8
17:49:49.824 -> 323s953:MAC rxDone
17:49:49.835 -> [RX] port=1 size=1
17:49:49.841 -> [RX] payload: 00 
17:49:49.848 -> [CMD] Simple command received: cmd=0x00, size=1
17:49:49.854 -> [CMD] Unknown simple command: 0x00
17:49:49.861 -> 323s960:RX_C on freq 923300000 Hz at DR 8
17:53:32.088 -> 546s261:MAC rxDone
17:53:32.099 -> 546s267:RX_C on freq 923300000 Hz at DR 8
17:54:01.417 -> 575s617:MAC rxDone
17:54:01.422 -> [RX] port=1 size=1
17:54:01.425 -> [RX] payload: 00 
17:54:01.430 -> [CMD] Simple command received: cmd=0x00, size=1
17:54:01.492 -> [CMD] Unknown simple command: 0x00
17:54:01.500 -> 575s625:RX_C on freq 923300000 Hz at DR 8
17:54:47.959 -> 622s174:MAC rxDone
17:54:48.016 -> 622s180:RX_C on freq 923300000 Hz at DR 8
17:55:33.889 -> 668s068:MAC rxDone
17:55:33.891 -> [RX] port=1 size=1
17:55:33.922 -> [RX] payload: 00 
17:55:33.949 -> [CMD] Simple command received: cmd=0x00, size=1
17:55:33.974 -> [CMD] Unknown simple command: 0x00
17:55:34.001 -> 668s076:RX_C on freq 923300000 Hz at DR 8
17:56:47.538 -> 741s757:MAC rxDone
17:56:47.555 -> 741s763:RX_C on freq 923300000 Hz at DR 8
17:56:57.661 -> 751s857:MAC rxDone
17:56:57.676 -> 751s863:RX_C on freq 923300000 Hz at DR 8
17:58:27.216 -> 841s446:MAC rxDone
17:58:27.238 -> 841s452:RX_C on freq 923300000 Hz at DR 8
17:59:03.230 -> 877s459:MAC rxDone
17:59:03.247 -> 877s465:RX_C on freq 923300000 Hz at DR 8
18:00:00.416 -> 934s667:MAC rxDone
18:00:00.430 -> 934s673:RX_C on freq 923300000 Hz at DR 8
18:00:01.410 -> 935s672:MAC rxDone
18:00:01.428 -> 935s678:RX_C on freq 923300000 Hz at DR 8
18:00:02.451 -> 936s682:MAC rxDone
18:00:02.468 -> 936s688:RX_C on freq 923300000 Hz at DR 8
18:00:03.503 -> 937s727:MAC rxDone
18:00:03.513 -> 937s734:RX_C on freq 923300000 Hz at DR 8
18:00:04.542 -> 938s774:MAC rxDone
18:00:04.552 -> 938s780:RX_C on freq 923300000 Hz at DR 8
18:00:05.563 -> 939s815:MAC rxDone
18:00:05.579 -> 939s821:RX_C on freq 923300000 Hz at DR 8
18:00:06.563 -> 940s827:MAC rxDone
18:00:06.585 -> 940s833:RX_C on freq 923300000 Hz at DR 8
18:00:07.666 -> 941s899:MAC rxDone
18:00:07.689 -> 941s905:RX_C on freq 923300000 Hz at DR 8
18:00:08.663 -> 942s916:MAC rxDone
18:00:08.673 -> 942s922:RX_C on freq 923300000 Hz at DR 8
18:00:09.848 -> 944s080:MAC rxDone
18:00:09.864 -> 944s085:RX_C on freq 923300000 Hz at DR 8
18:00:10.743 -> 944s980:MAC rxDone
18:00:10.756 -> 944s986:RX_C on freq 923300000 Hz at DR 8
18:00:11.739 -> 945s985:MAC rxDone
18:00:11.756 -> 945s991:RX_C on freq 923300000 Hz at DR 8
18:00:12.021 -> [LORA] Next period armed: 900000 ms (phaseOnce=3244)
18:00:12.034 -> 
18:00:12.046 -> [PIMA] Uplink routine
18:00:12.067 -> [PIMA] pima_read_cycle: start (burstMax=60)
18:00:12.079 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:00:12.805 -> 947s032:MAC rxDone
18:00:13.273 -> 947s533:MAC rxDone
18:00:13.490 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:13.857 -> 948s081:MAC rxDone
18:00:14.829 -> 949s067:MAC rxDone
18:00:14.943 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:15.870 -> 950s112:MAC rxDone
18:00:16.383 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:16.899 -> 951s135:MAC rxDone
18:00:17.874 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:18.038 -> 952s268:MAC rxDone
18:00:19.009 -> 953s268:MAC rxDone
18:00:19.325 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:19.643 -> 953s892:MAC rxDone
18:00:19.807 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:00:19.825 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:00:19.857 -> [PIMA] pima_read_cycle: attempt 1 -> fail
18:00:19.880 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:00:20.056 -> 954s298:MAC rxDone
18:00:20.713 -> 954s946:MAC rxDone
18:00:21.027 -> 955s289:MAC rxDone
18:00:21.291 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:22.067 -> 956s309:MAC rxDone
18:00:22.737 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:23.108 -> 957s356:MAC rxDone
18:00:24.133 -> 958s384:MAC rxDone
18:00:24.196 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:24.814 -> 959s057:MAC rxDone
18:00:25.181 -> 959s423:MAC rxDone
18:00:25.649 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:26.186 -> 960s435:MAC rxDone
18:00:27.153 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:00:27.220 -> 961s472:MAC rxDone
18:00:27.639 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:00:27.647 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:00:27.661 -> [PIMA] pima_read_cycle: attempt 2 -> fail
18:00:27.669 -> [PIMA] pima_read_cycle: overall timeout reached
18:00:27.689 -> [PIMA] pima_read_cycle: no packet captured
18:00:27.710 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
18:00:27.737 -> 961s873:TX on freq 917400000 Hz at DR 5
18:00:27.761 -> [LORA] OnTxData: status=1, DR=5, UplinkCounter=3, Channel=11
18:00:27.774 -> 961s883:RX_C on freq 923300000 Hz at DR 8
18:00:28.291 -> 962s525:MAC rxDone
18:00:28.311 -> 962s532:RX_C on freq 923300000 Hz at DR 8
18:00:31.615 -> 965s877:MAC txTimeOut
18:00:31.622 -> 965s879:MAC rxDone
18:00:31.682 -> 965s891:RX_C on freq 923300000 Hz at DR 8
18:00:36.880 -> 971s114:MAC rxDone
18:00:36.886 -> 971s120:RX_C on freq 923300000 Hz at DR 8
18:00:38.298 -> 972s545:MAC rxDone
18:00:38.304 -> 972s551:RX_C on freq 923300000 Hz at DR 8
18:00:43.307 -> 977s541:MAC rxDone
18:00:43.318 -> 977s547:RX_C on freq 923300000 Hz at DR 8
18:00:51.446 -> 985s717:MAC rxDone
18:00:51.464 -> 985s723:RX_C on freq 923300000 Hz at DR 8
18:00:55.481 -> 989s736:MAC rxDone
18:00:55.505 -> 989s742:RX_C on freq 923300000 Hz at DR 8
18:00:56.743 -> 990s973:MAC rxDone
18:00:56.749 -> [RX] port=1 size=1
18:00:56.754 -> [RX] payload: 00 
18:00:56.763 -> [CMD] Simple command received: cmd=0x00, size=1
18:00:56.769 -> [CMD] Unknown simple command: 0x00
18:00:56.774 -> 990s981:RX_C on freq 923300000 Hz at DR 8
18:00:58.141 -> 992s373:MAC rxDone
18:00:58.147 -> 992s379:RX_C on freq 923300000 Hz at DR 8
18:01:59.640 -> 1053s929:MAC rxDone
18:01:59.694 -> 1053s935:RX_C on freq 923300000 Hz at DR 8
18:04:15.007 -> 1189s319:MAC rxDone
18:04:15.070 -> [RX] port=1 size=1
18:04:15.076 -> [RX] payload: 00 
18:04:15.092 -> [CMD] Simple command received: cmd=0x00, size=1
18:04:15.103 -> [CMD] Unknown simple command: 0x00
18:04:15.109 -> 1189s327:RX_C on freq 923300000 Hz at DR 8
18:05:31.913 -> 1266s231:MAC rxDone
18:05:31.922 -> 1266s237:RX_C on freq 923300000 Hz at DR 8
18:05:54.371 -> 1288s657:MAC rxDone
18:05:54.377 -> [RX] port=1 size=1
18:05:54.390 -> [RX] payload: 00 
18:05:54.400 -> [CMD] Simple command received: cmd=0x00, size=1
18:05:54.412 -> [CMD] Unknown simple command: 0x00
18:05:54.418 -> 1288s665:RX_C on freq 923300000 Hz at DR 8
18:08:53.327 -> 1467s641:MAC rxDone
18:08:53.334 -> 1467s648:RX_C on freq 923300000 Hz at DR 8
18:11:31.313 -> 1625s680:MAC rxDone
18:11:31.323 -> 1625s686:RX_C on freq 923300000 Hz at DR 8
18:14:56.076 -> 1830s472:MAC rxDone
18:14:56.082 -> 1830s478:RX_C on freq 923300000 Hz at DR 8
18:15:11.872 -> [LORA] Next period armed: 900000 ms (phaseOnce=3244)
18:15:11.878 -> 
18:15:11.891 -> [PIMA] Uplink routine
18:15:11.901 -> [PIMA] pima_read_cycle: start (burstMax=60)
18:15:11.913 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:15:13.328 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:14.801 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:16.271 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:17.692 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:19.159 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:19.674 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:15:19.687 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:15:19.696 -> [PIMA] pima_read_cycle: attempt 1 -> fail
18:15:19.699 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:15:20.969 -> 1855s354:MAC rxDone
18:15:21.126 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:21.995 -> 1856s388:MAC rxDone
18:15:22.611 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:24.085 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:25.506 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:26.970 -> 1861s359:MAC rxDone
18:15:26.977 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:15:27.338 -> 1861s751:MAC rxDone
18:15:27.495 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:15:27.503 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:15:27.511 -> [PIMA] pima_read_cycle: attempt 2 -> fail
18:15:27.519 -> [PIMA] pima_read_cycle: overall timeout reached
18:15:27.528 -> [PIMA] pima_read_cycle: no packet captured
18:15:27.537 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
18:15:27.542 -> 1861s873:TX on freq 916800000 Hz at DR 5
18:15:27.552 -> [LORA] OnTxData: status=1, DR=5, UplinkCounter=4, Channel=8
18:15:27.557 -> 1861s883:RX_C on freq 923300000 Hz at DR 8
18:15:28.019 -> 1862s434:MAC rxDone
18:15:28.076 -> 1862s440:RX_C on freq 923300000 Hz at DR 8
18:15:29.341 -> 1863s750:MAC rxDone
18:15:29.346 -> 1863s756:RX_C on freq 923300000 Hz at DR 8
18:15:29.911 -> 1864s326:MAC rxDone
18:15:29.968 -> 1864s332:RX_C on freq 923300000 Hz at DR 8
18:15:31.487 -> 1865s877:MAC txTimeOut
18:15:33.460 -> 1867s875:MAC rxDone
18:15:33.516 -> 1867s882:RX_C on freq 923300000 Hz at DR 8
18:15:39.477 -> 1873s878:MAC rxDone
18:15:39.483 -> 1873s884:RX_C on freq 923300000 Hz at DR 8
18:15:53.366 -> 1887s759:MAC rxDone
18:15:53.375 -> 1887s765:RX_C on freq 923300000 Hz at DR 8
18:19:07.708 -> 2082s158:MAC rxDone
18:19:07.715 -> 2082s158:IRQ_CRC_ERROR
18:19:07.776 -> 2082s165:RX_C on freq 923300000 Hz at DR 8
18:23:17.531 -> 2332s017:MAC rxDone
18:23:17.536 -> 2332s023:RX_C on freq 923300000 Hz at DR 8
18:24:39.154 -> 2413s658:MAC rxDone
18:24:39.213 -> 2413s664:RX_C on freq 923300000 Hz at DR 8
18:26:06.372 -> 2500s863:MAC rxDone
18:26:06.382 -> 2500s869:RX_C on freq 923300000 Hz at DR 8
18:27:03.232 -> 2557s759:MAC rxDone
18:27:03.289 -> 2557s765:RX_C on freq 923300000 Hz at DR 8
18:30:05.707 -> 2740s238:MAC rxDone
18:30:05.716 -> 2740s244:RX_C on freq 923300000 Hz at DR 8
18:30:11.727 -> [LORA] Next period armed: 900000 ms (phaseOnce=3244)
18:30:11.734 -> 
18:30:11.746 -> [PIMA] Uplink routine
18:30:11.755 -> [PIMA] pima_read_cycle: start (burstMax=60)
18:30:11.764 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:30:13.180 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:14.649 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:16.120 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:17.589 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:19.054 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:19.515 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:30:19.521 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:30:19.530 -> [PIMA] pima_read_cycle: attempt 1 -> fail
18:30:19.541 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:30:19.752 -> 2754s315:MAC rxDone
18:30:20.972 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:21.030 -> 2755s564:MAC rxDone
18:30:22.451 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:23.922 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:25.391 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:26.860 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:30:27.323 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:30:27.328 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:30:27.337 -> [PIMA] pima_read_cycle: attempt 2 -> fail
18:30:27.343 -> [PIMA] pima_read_cycle: overall timeout reached
18:30:27.404 -> [PIMA] pima_read_cycle: no packet captured
18:30:27.410 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
18:30:27.420 -> 2761s873:TX on freq 918200000 Hz at DR 5
18:30:27.430 -> [LORA] OnTxData: status=1, DR=5, UplinkCounter=5, Channel=15
18:30:27.440 -> 2761s883:RX_C on freq 923300000 Hz at DR 8
18:30:29.565 -> 2764s125:MAC rxDone
18:30:29.623 -> 2764s131:RX_C on freq 923300000 Hz at DR 8
18:30:30.639 -> 2765s176:MAC rxDone
18:30:30.644 -> 2765s183:RX_C on freq 923300000 Hz at DR 8
18:30:30.905 -> 2765s449:MAC rxDone
18:30:30.910 -> 2765s456:RX_C on freq 923300000 Hz at DR 8
18:30:31.324 -> 2765s877:MAC txTimeOut
18:30:34.706 -> 2769s270:MAC rxDone
18:30:34.767 -> 2769s276:RX_C on freq 923300000 Hz at DR 8
18:30:36.188 -> 2770s746:MAC rxDone
18:30:36.194 -> 2770s751:RX_C on freq 923300000 Hz at DR 8
18:30:37.161 -> 2771s687:MAC rxDone
18:30:37.168 -> 2771s693:RX_C on freq 923300000 Hz at DR 8
18:30:37.430 -> 2771s955:MAC rxDone
18:30:37.438 -> 2771s960:RX_C on freq 923300000 Hz at DR 8
18:30:38.456 -> 2772s992:MAC rxDone
18:30:38.465 -> 2772s998:RX_C on freq 923300000 Hz at DR 8
18:30:39.584 -> 2774s145:MAC rxDone
18:30:39.592 -> 2774s151:RX_C on freq 923300000 Hz at DR 8
18:30:46.712 -> 2781s244:MAC rxDone
18:30:46.719 -> 2781s250:RX_C on freq 923300000 Hz at DR 8
18:30:47.435 -> 2781s965:MAC rxDone
18:30:47.442 -> 2781s971:RX_C on freq 923300000 Hz at DR 8
18:30:54.958 -> 2789s486:MAC rxDone
18:30:54.964 -> 2789s492:RX_C on freq 923300000 Hz at DR 8
18:31:30.878 -> 2825s429:MAC rxDone
18:31:30.884 -> 2825s435:RX_C on freq 923300000 Hz at DR 8
18:34:25.478 -> [BOOT] APP V1.2.0
18:34:25.486 -> [BOOT] LoRaWAN MW V2.4.0
18:34:25.495 -> [BOOT] Radio PHY V1.2.0
18:34:25.505 -> [LORA] NVM data restored
18:34:25.514 -> ###### IDs  ######
18:34:25.524 -> ###### DevEui:      AC:1F:09:26:00:2F:00:03
18:34:25.532 -> ###### AppEui:      00:00:00:00:00:00:00:00
18:34:25.542 -> ###### DevAddr:     05:6C:52:23
18:34:25.548 -> [LORA] AU915 sub-band 2 applied
18:34:25.557 -> [HP] Loaded from flash: DISABLED (raw=0)
18:34:25.616 -> [OTAA] Period loaded from flash: 900000 ms
18:34:25.623 -> [HP] High Precision Mode: DISABLED (fromFlash=1)
18:34:25.632 -> [OTAA] Base period at boot: 900000 ms (fromFlash=1)
18:34:25.641 -> [BOOT] Waiting 5 seconds before JOIN...
18:34:30.497 -> [KEYS] Loaded from flash
18:34:30.503 -> DEVEUI:ac1f0926002f0003
18:34:30.512 -> APPKEY:f2839693c180a9df89412e3098ba5a43
18:34:30.521 -> MODEL:ST-EAM-01B
18:34:30.581 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
18:34:30.592 -> 5s051:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
18:34:30.609 -> [LORA] Starting join (OTAA)
18:34:30.615 -> 5s058:TX on freq 915200000 Hz at DR 2
18:34:30.874 -> 5s431:MAC txDone
18:34:35.874 -> 10s408:RX_1 on freq 923300000 Hz at DR 10
18:34:35.933 -> 10s458:IRQ_RX_TX_TIMEOUT
18:34:35.939 -> 10s458:MAC rxTimeOut
18:34:36.857 -> 11s419:RX_2 on freq 923300000 Hz at DR 8
18:34:36.917 -> 11s485:IRQ_RX_TX_TIMEOUT
18:34:36.923 -> 11s486:MAC rxTimeOut
18:34:36.984 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
18:34:36.990 -> 
18:34:36.999 -> [LORA] JOIN FAILED (status=-1) count=1
18:34:37.009 -> [LORA] Rejoin scheduled
18:34:46.954 -> 21s492:TX on freq 917800000 Hz at DR 2
18:34:46.961 -> [LORA] Rejoin busy -> retry in 5000 ms
18:34:47.325 -> 21s865:MAC txDone
18:34:51.972 -> [LORA] Rejoin busy -> retry in 5000 ms
18:34:52.283 -> 26s842:RX_1 on freq 926300000 Hz at DR 10
18:34:52.442 -> 26s981:MAC rxDone
18:34:52.449 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
18:34:52.458 -> 
18:34:52.465 -> [LORA] JOINED (OTAA)
18:34:52.474 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
18:34:52.484 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
18:34:52.494 -> ###### NwkSKey:     D3:04:CD:03:40:9D:8A:54:06:52:8A:C4:FC:9F:AB:FB
18:34:52.503 -> ###### AppSKey:     76:11:55:49:08:8F:D5:7C:C2:79:93:B6:B7:D1:7E:6A
18:35:00.436 -> [PIMA] B1 warmup uplink
18:35:00.444 -> 
18:35:00.454 -> [PIMA] Uplink routine
18:35:00.464 -> [BOOT] Sending initial warmup byte (B1)
18:35:00.472 -> 34s991:TX on freq 917400000 Hz at DR 2
18:35:00.734 -> 35s283:MAC txDone
18:35:05.734 -> 40s259:RX_1 on freq 925100000 Hz at DR 10
18:35:05.791 -> 40s368:MAC rxDone
18:35:05.847 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=11
18:35:05.855 -> [RX] port=0 size=0
18:35:08.435 -> [PIMA] First read after boot
18:35:08.441 -> [PIMA] Changing to OTAA_PERIOD mode
18:35:08.451 -> [LORA] Phase offset applied once: 2037 ms (base=900000 ms)
18:35:08.460 -> 
18:35:08.469 -> [PIMA] Uplink routine
18:35:08.477 -> [PIMA] pima_read_cycle: start (burstMax=60)
18:35:08.487 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:35:09.908 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:11.376 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:12.847 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:14.319 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:15.738 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:16.250 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:35:16.258 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:35:16.267 -> [PIMA] pima_read_cycle: attempt 1 -> fail
18:35:16.277 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:35:17.697 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:19.169 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:20.638 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:22.108 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:23.579 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:35:24.036 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:35:24.092 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:35:24.097 -> [PIMA] pima_read_cycle: attempt 2 -> fail
18:35:24.107 -> [PIMA] pima_read_cycle: overall timeout reached
18:35:24.117 -> [PIMA] pima_read_cycle: no packet captured
18:35:24.126 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
18:35:24.135 -> 58s617:TX on freq 918000000 Hz at DR 5
18:35:24.195 -> 58s760:MAC txDone
18:35:29.194 -> 63s734:RX_1 on freq 926900000 Hz at DR 13
18:35:29.200 -> 63s763:IRQ_RX_TX_TIMEOUT
18:35:29.209 -> 63s764:MAC rxTimeOut
18:35:30.178 -> 64s749:RX_2 on freq 923300000 Hz at DR 8
18:35:30.236 -> 64s814:IRQ_RX_TX_TIMEOUT
18:35:30.292 -> 64s815:MAC rxTimeOut
18:35:30.299 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=14
18:50:10.338 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
18:50:10.346 -> 
18:50:10.355 -> [PIMA] Uplink routine
18:50:10.363 -> [PIMA] pima_read_cycle: start (burstMax=60)
18:50:10.373 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:50:11.796 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:13.268 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:14.737 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:16.205 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:17.625 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:18.135 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:50:18.141 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:50:18.150 -> [PIMA] pima_read_cycle: attempt 1 -> fail
18:50:18.158 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
18:50:19.578 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:21.049 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:22.524 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:23.992 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:25.463 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
18:50:25.924 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
18:50:25.982 -> [PIMA] Base frame 0x02 search timeout (no base found)
18:50:25.989 -> [PIMA] pima_read_cycle: attempt 2 -> fail
18:50:25.999 -> [PIMA] pima_read_cycle: overall timeout reached
18:50:26.009 -> [PIMA] pima_read_cycle: no packet captured
18:50:26.018 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
18:50:26.027 -> 960s653:TX on freq 917000000 Hz at DR 5
18:50:26.088 -> 960s791:MAC txDone
18:50:31.040 -> 965s765:RX_1 on freq 923900000 Hz at DR 13
18:50:31.097 -> 965s805:MAC rxDone
18:50:31.103 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=3, Channel=9
18:50:31.110 -> [RX] port=0 size=0
19:05:10.180 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
19:05:10.186 -> 
19:05:10.195 -> [PIMA] Uplink routine
19:05:10.205 -> [PIMA] pima_read_cycle: start (burstMax=60)
19:05:10.215 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:05:11.639 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:13.107 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:14.575 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:16.042 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:17.511 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:17.972 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:05:17.979 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:05:18.039 -> [PIMA] pima_read_cycle: attempt 1 -> fail
19:05:18.045 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:05:19.466 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:20.937 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:22.408 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:23.825 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:25.294 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:05:25.804 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:05:25.812 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:05:25.822 -> [PIMA] pima_read_cycle: attempt 2 -> fail
19:05:25.831 -> [PIMA] pima_read_cycle: overall timeout reached
19:05:25.841 -> [PIMA] pima_read_cycle: no packet captured
19:05:25.851 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
19:05:25.859 -> 1860s653:TX on freq 916800000 Hz at DR 5
19:05:25.920 -> 1860s791:MAC txDone
19:05:30.919 -> 1865s765:RX_1 on freq 923300000 Hz at DR 13
19:05:30.975 -> 1865s804:MAC rxDone
19:05:30.980 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=4, Channel=8
19:05:30.989 -> [RX] port=0 size=0
19:20:10.017 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
19:20:10.025 -> 
19:20:10.033 -> [PIMA] Uplink routine
19:20:10.044 -> [PIMA] pima_read_cycle: start (burstMax=60)
19:20:10.103 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:20:11.473 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:12.942 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:14.414 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:15.885 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:17.357 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:17.867 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:20:17.873 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:20:17.881 -> [PIMA] pima_read_cycle: attempt 1 -> fail
19:20:17.888 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:20:19.308 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:20.779 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:22.248 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:23.720 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:25.189 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:20:25.650 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:20:25.659 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:20:25.667 -> [PIMA] pima_read_cycle: attempt 2 -> fail
19:20:25.676 -> [PIMA] pima_read_cycle: overall timeout reached
19:20:25.684 -> [PIMA] pima_read_cycle: no packet captured
19:20:25.745 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
19:20:25.752 -> 2760s652:TX on freq 917200000 Hz at DR 5
19:20:25.812 -> 2760s791:MAC txDone
19:20:30.761 -> 2765s764:RX_1 on freq 924500000 Hz at DR 13
19:20:30.819 -> 2765s803:MAC rxDone
19:20:30.829 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=5, Channel=10
19:20:30.839 -> [RX] port=0 size=0
19:35:09.877 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
19:35:09.882 -> 
19:35:09.894 -> [PIMA] Uplink routine
19:35:09.905 -> [PIMA] pima_read_cycle: start (burstMax=60)
19:35:09.916 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:35:11.339 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:12.809 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:14.280 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:15.751 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:17.223 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:17.685 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:35:17.691 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:35:17.699 -> [PIMA] pima_read_cycle: attempt 1 -> fail
19:35:17.708 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:35:19.182 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:20.606 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:22.075 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:23.547 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:25.019 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:35:25.480 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:35:25.542 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:35:25.547 -> [PIMA] pima_read_cycle: attempt 2 -> fail
19:35:25.557 -> [PIMA] pima_read_cycle: overall timeout reached
19:35:25.566 -> [PIMA] pima_read_cycle: no packet captured
19:35:25.577 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
19:35:25.588 -> 3660s653:TX on freq 917600000 Hz at DR 5
19:35:25.648 -> 3660s791:MAC txDone
19:35:30.601 -> 3665s765:RX_1 on freq 925700000 Hz at DR 13
19:35:30.660 -> 3665s806:IRQ_RX_TX_TIMEOUT
19:35:30.668 -> 3665s806:MAC rxTimeOut
19:35:31.637 -> 3666s780:RX_2 on freq 923300000 Hz at DR 8
19:35:31.696 -> 3666s845:IRQ_RX_TX_TIMEOUT
19:35:31.704 -> 3666s846:MAC rxTimeOut
19:35:31.714 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=6, Channel=12
19:50:09.727 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
19:50:09.735 -> 
19:50:09.747 -> [PIMA] Uplink routine
19:50:09.758 -> [PIMA] pima_read_cycle: start (burstMax=60)
19:50:09.767 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:50:11.189 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:12.660 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:14.133 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:15.603 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:17.074 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:17.534 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:50:17.541 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:50:17.550 -> [PIMA] pima_read_cycle: attempt 1 -> fail
19:50:17.561 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
19:50:18.985 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:20.456 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:21.924 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:23.397 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:24.872 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
19:50:25.333 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
19:50:25.393 -> [PIMA] Base frame 0x02 search timeout (no base found)
19:50:25.402 -> [PIMA] pima_read_cycle: attempt 2 -> fail
19:50:25.411 -> [PIMA] pima_read_cycle: overall timeout reached
19:50:25.422 -> [PIMA] pima_read_cycle: no packet captured
19:50:25.432 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
19:50:25.441 -> 4560s653:TX on freq 918200000 Hz at DR 5
19:50:25.501 -> 4560s791:MAC txDone
19:50:30.449 -> 4565s765:RX_1 on freq 927500000 Hz at DR 13
19:50:30.507 -> 4565s804:MAC rxDone
19:50:30.517 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=7, Channel=15
19:50:30.527 -> [RX] port=0 size=0
20:05:09.564 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
20:05:09.572 -> 
20:05:09.582 -> [PIMA] Uplink routine
20:05:09.642 -> [PIMA] pima_read_cycle: start (burstMax=60)
20:05:09.648 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:05:11.069 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:12.491 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:13.960 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:15.426 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:16.897 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:17.409 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:05:17.416 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:05:17.426 -> [PIMA] pima_read_cycle: attempt 1 -> fail
20:05:17.434 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:05:18.857 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:20.327 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:21.795 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:23.266 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:24.737 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:05:25.199 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:05:25.207 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:05:25.215 -> [PIMA] pima_read_cycle: attempt 2 -> fail
20:05:25.226 -> [PIMA] pima_read_cycle: overall timeout reached
20:05:25.286 -> [PIMA] pima_read_cycle: no packet captured
20:05:25.294 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
20:05:25.304 -> 5460s653:TX on freq 917800000 Hz at DR 5
20:05:25.365 -> 5460s791:MAC txDone
20:05:30.318 -> 5465s765:RX_1 on freq 926300000 Hz at DR 13
20:05:30.375 -> 5465s806:IRQ_RX_TX_TIMEOUT
20:05:30.382 -> 5465s806:MAC rxTimeOut
20:05:31.350 -> 5466s780:RX_2 on freq 923300000 Hz at DR 8
20:05:31.408 -> 5466s845:IRQ_RX_TX_TIMEOUT
20:05:31.417 -> 5466s846:MAC rxTimeOut
20:05:31.426 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=8, Channel=13
20:20:09.451 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
20:20:09.459 -> 
20:20:09.468 -> [PIMA] Uplink routine
20:20:09.475 -> [PIMA] pima_read_cycle: start (burstMax=60)
20:20:09.486 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:20:10.907 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:12.376 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:13.848 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:15.318 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:16.741 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:17.252 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:20:17.261 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:20:17.269 -> [PIMA] pima_read_cycle: attempt 1 -> fail
20:20:17.274 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:20:18.692 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:20.165 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:21.634 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:23.105 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:24.576 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:20:25.036 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:20:25.093 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:20:25.099 -> [PIMA] pima_read_cycle: attempt 2 -> fail
20:20:25.108 -> [PIMA] pima_read_cycle: overall timeout reached
20:20:25.114 -> [PIMA] pima_read_cycle: no packet captured
20:20:25.124 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
20:20:25.135 -> 6360s653:TX on freq 918000000 Hz at DR 5
20:20:25.196 -> 6360s791:MAC txDone
20:20:30.195 -> 6365s765:RX_1 on freq 926900000 Hz at DR 13
20:20:30.202 -> 6365s806:IRQ_RX_TX_TIMEOUT
20:20:30.211 -> 6365s806:MAC rxTimeOut
20:20:31.179 -> 6366s780:RX_2 on freq 923300000 Hz at DR 8
20:20:31.236 -> 6366s845:IRQ_RX_TX_TIMEOUT
20:20:31.244 -> 6366s846:MAC rxTimeOut
20:20:31.253 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=9, Channel=14
20:35:09.280 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
20:35:09.287 -> 
20:35:09.297 -> [PIMA] Uplink routine
20:35:09.305 -> [PIMA] pima_read_cycle: start (burstMax=60)
20:35:09.313 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:35:10.734 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:12.206 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:13.679 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:15.150 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:16.622 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:17.085 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:35:17.094 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:35:17.103 -> [PIMA] pima_read_cycle: attempt 1 -> fail
20:35:17.162 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:35:18.580 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:20.051 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:21.471 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:22.940 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:24.410 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:35:24.923 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:35:24.929 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:35:24.938 -> [PIMA] pima_read_cycle: attempt 2 -> fail
20:35:24.949 -> [PIMA] pima_read_cycle: overall timeout reached
20:35:24.957 -> [PIMA] pima_read_cycle: no packet captured
20:35:24.966 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
20:35:24.975 -> 7260s653:TX on freq 916800000 Hz at DR 5
20:35:25.034 -> 7260s791:MAC txDone
20:35:30.035 -> 7265s765:RX_1 on freq 923300000 Hz at DR 13
20:35:30.092 -> 7265s806:IRQ_RX_TX_TIMEOUT
20:35:30.099 -> 7265s806:MAC rxTimeOut
20:35:31.018 -> 7266s780:RX_2 on freq 923300000 Hz at DR 8
20:35:31.127 -> 7266s845:IRQ_RX_TX_TIMEOUT
20:35:31.133 -> 7266s846:MAC rxTimeOut
20:35:31.144 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=10, Channel=8
20:50:09.132 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
20:50:09.139 -> 
20:50:09.148 -> [PIMA] Uplink routine
20:50:09.157 -> [PIMA] pima_read_cycle: start (burstMax=60)
20:50:09.166 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:50:10.590 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:12.059 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:13.528 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:14.999 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:16.467 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:16.930 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:50:16.939 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:50:17.000 -> [PIMA] pima_read_cycle: attempt 1 -> fail
20:50:17.008 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
20:50:18.428 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:19.899 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:21.319 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:22.793 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:24.262 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
20:50:24.775 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
20:50:24.783 -> [PIMA] Base frame 0x02 search timeout (no base found)
20:50:24.794 -> [PIMA] pima_read_cycle: attempt 2 -> fail
20:50:24.802 -> [PIMA] pima_read_cycle: overall timeout reached
20:50:24.812 -> [PIMA] pima_read_cycle: no packet captured
20:50:24.822 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
20:50:24.833 -> 8160s653:TX on freq 917400000 Hz at DR 5
20:50:24.896 -> 8160s791:MAC txDone
20:50:29.897 -> 8165s765:RX_1 on freq 925100000 Hz at DR 13
20:50:29.906 -> 8165s806:IRQ_RX_TX_TIMEOUT
20:50:29.914 -> 8165s806:MAC rxTimeOut
20:50:30.885 -> 8166s780:RX_2 on freq 923300000 Hz at DR 8
20:50:30.943 -> 8166s845:IRQ_RX_TX_TIMEOUT
20:50:30.950 -> 8166s846:MAC rxTimeOut
20:50:30.958 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=11, Channel=11
21:05:08.992 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
21:05:09.000 -> 
21:05:09.008 -> [PIMA] Uplink routine
21:05:09.018 -> [PIMA] pima_read_cycle: start (burstMax=60)
21:05:09.025 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:05:10.445 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:11.914 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:13.383 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:14.855 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:16.326 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:16.788 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:05:16.794 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:05:16.804 -> [PIMA] pima_read_cycle: attempt 1 -> fail
21:05:16.814 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:05:18.287 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:19.710 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:21.182 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:22.649 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:24.118 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:05:24.632 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:05:24.640 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:05:24.650 -> [PIMA] pima_read_cycle: attempt 2 -> fail
21:05:24.660 -> [PIMA] pima_read_cycle: overall timeout reached
21:05:24.670 -> [PIMA] pima_read_cycle: no packet captured
21:05:24.679 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
21:05:24.688 -> 9060s653:TX on freq 917200000 Hz at DR 5
21:05:24.749 -> 9060s791:MAC txDone
21:05:29.750 -> 9065s765:RX_1 on freq 924500000 Hz at DR 13
21:05:29.756 -> 9065s806:IRQ_RX_TX_TIMEOUT
21:05:29.764 -> 9065s806:MAC rxTimeOut
21:05:30.730 -> 9066s780:RX_2 on freq 923300000 Hz at DR 8
21:05:30.786 -> 9066s845:IRQ_RX_TX_TIMEOUT
21:05:30.793 -> 9066s846:MAC rxTimeOut
21:05:30.853 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=12, Channel=10
21:20:08.816 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
21:20:08.823 -> 
21:20:08.834 -> [PIMA] Uplink routine
21:20:08.895 -> [PIMA] pima_read_cycle: start (burstMax=60)
21:20:08.901 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:20:10.322 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:11.745 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:13.213 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:14.684 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:16.153 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:16.669 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:20:16.676 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:20:16.684 -> [PIMA] pima_read_cycle: attempt 1 -> fail
21:20:16.694 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:20:18.114 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:19.586 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:21.058 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:22.529 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:23.949 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:20:24.460 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:20:24.467 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:20:24.476 -> [PIMA] pima_read_cycle: attempt 2 -> fail
21:20:24.486 -> [PIMA] pima_read_cycle: overall timeout reached
21:20:24.495 -> [PIMA] pima_read_cycle: no packet captured
21:20:24.505 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
21:20:24.565 -> 9960s653:TX on freq 918200000 Hz at DR 5
21:20:24.622 -> 9960s791:MAC txDone
21:20:29.571 -> 9965s765:RX_1 on freq 927500000 Hz at DR 13
21:20:29.631 -> 9965s806:IRQ_RX_TX_TIMEOUT
21:20:29.639 -> 9965s806:MAC rxTimeOut
21:20:30.609 -> 9966s780:RX_2 on freq 923300000 Hz at DR 8
21:20:30.666 -> 9966s845:IRQ_RX_TX_TIMEOUT
21:20:30.671 -> 9966s846:MAC rxTimeOut
21:20:30.681 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=13, Channel=15
21:35:08.663 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
21:35:08.669 -> 
21:35:08.729 -> [PIMA] Uplink routine
21:35:08.735 -> [PIMA] pima_read_cycle: start (burstMax=60)
21:35:08.745 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:35:10.167 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:11.636 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:13.107 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:14.527 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:15.997 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:16.506 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:35:16.516 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:35:16.528 -> [PIMA] pima_read_cycle: attempt 1 -> fail
21:35:16.537 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:35:17.960 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:19.431 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:20.902 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:22.376 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:23.839 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:35:24.302 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:35:24.308 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:35:24.318 -> [PIMA] pima_read_cycle: attempt 2 -> fail
21:35:24.326 -> [PIMA] pima_read_cycle: overall timeout reached
21:35:24.387 -> [PIMA] pima_read_cycle: no packet captured
21:35:24.393 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
21:35:24.403 -> 10860s652:TX on freq 917600000 Hz at DR 5
21:35:24.460 -> 10860s791:MAC txDone
21:35:29.409 -> 10865s764:RX_1 on freq 925700000 Hz at DR 13
21:35:29.467 -> 10865s805:IRQ_RX_TX_TIMEOUT
21:35:29.474 -> 10865s805:MAC rxTimeOut
21:35:30.442 -> 10866s779:RX_2 on freq 923300000 Hz at DR 8
21:35:30.500 -> 10866s844:IRQ_RX_TX_TIMEOUT
21:35:30.505 -> 10866s845:MAC rxTimeOut
21:35:30.514 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=14, Channel=12
21:50:08.547 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
21:50:08.552 -> 
21:50:08.561 -> [PIMA] Uplink routine
21:50:08.570 -> [PIMA] pima_read_cycle: start (burstMax=60)
21:50:08.579 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:50:10.000 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:11.470 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:12.939 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:14.411 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:15.881 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:16.344 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:50:16.352 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:50:16.361 -> [PIMA] pima_read_cycle: attempt 1 -> fail
21:50:16.371 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
21:50:17.792 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:19.263 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:20.732 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:22.204 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:23.672 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
21:50:24.184 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
21:50:24.190 -> [PIMA] Base frame 0x02 search timeout (no base found)
21:50:24.200 -> [PIMA] pima_read_cycle: attempt 2 -> fail
21:50:24.209 -> [PIMA] pima_read_cycle: overall timeout reached
21:50:24.218 -> [PIMA] pima_read_cycle: no packet captured
21:50:24.225 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
21:50:24.233 -> 11760s653:TX on freq 917000000 Hz at DR 5
21:50:24.294 -> 11760s791:MAC txDone
21:50:29.297 -> 11765s765:RX_1 on freq 923900000 Hz at DR 13
21:50:29.303 -> 11765s806:IRQ_RX_TX_TIMEOUT
21:50:29.312 -> 11765s806:MAC rxTimeOut
21:50:30.281 -> 11766s780:RX_2 on freq 923300000 Hz at DR 8
21:50:30.339 -> 11766s845:IRQ_RX_TX_TIMEOUT
21:50:30.345 -> 11766s846:MAC rxTimeOut
21:50:30.356 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=15, Channel=9
22:05:08.390 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
22:05:08.397 -> 
22:05:08.403 -> [PIMA] Uplink routine
22:05:08.411 -> [PIMA] pima_read_cycle: start (burstMax=60)
22:05:08.420 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:05:09.843 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:11.311 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:12.780 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:14.249 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:15.720 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:16.184 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:05:16.189 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:05:16.200 -> [PIMA] pima_read_cycle: attempt 1 -> fail
22:05:16.260 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:05:17.680 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:19.148 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:20.614 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:22.033 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:23.504 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:05:24.019 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:05:24.029 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:05:24.038 -> [PIMA] pima_read_cycle: attempt 2 -> fail
22:05:24.048 -> [PIMA] pima_read_cycle: overall timeout reached
22:05:24.056 -> [PIMA] pima_read_cycle: no packet captured
22:05:24.065 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
22:05:24.074 -> 12660s653:TX on freq 917600000 Hz at DR 5
22:05:24.135 -> 12660s791:MAC txDone
22:05:29.135 -> 12665s765:RX_1 on freq 925700000 Hz at DR 13
22:05:29.193 -> 12665s806:IRQ_RX_TX_TIMEOUT
22:05:29.199 -> 12665s806:MAC rxTimeOut
22:05:30.116 -> 12666s780:RX_2 on freq 923300000 Hz at DR 8
22:05:30.225 -> 12666s845:IRQ_RX_TX_TIMEOUT
22:05:30.230 -> 12666s846:MAC rxTimeOut
22:05:30.239 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=16, Channel=12
22:20:08.252 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
22:20:08.261 -> 
22:20:08.270 -> [PIMA] Uplink routine
22:20:08.279 -> [PIMA] pima_read_cycle: start (burstMax=60)
22:20:08.285 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:20:09.706 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:11.177 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:12.652 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:14.070 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:15.540 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:16.050 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:20:16.056 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:20:16.062 -> [PIMA] pima_read_cycle: attempt 1 -> fail
22:20:16.070 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:20:17.492 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:18.960 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:20.430 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:21.902 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:23.374 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:20:23.835 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:20:23.892 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:20:23.902 -> [PIMA] pima_read_cycle: attempt 2 -> fail
22:20:23.911 -> [PIMA] pima_read_cycle: overall timeout reached
22:20:23.924 -> [PIMA] pima_read_cycle: no packet captured
22:20:23.935 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
22:20:23.945 -> 13560s653:TX on freq 917400000 Hz at DR 5
22:20:24.005 -> 13560s791:MAC txDone
22:20:28.954 -> 13565s765:RX_1 on freq 925100000 Hz at DR 13
22:20:29.013 -> 13565s806:IRQ_RX_TX_TIMEOUT
22:20:29.018 -> 13565s806:MAC rxTimeOut
22:20:29.986 -> 13566s780:RX_2 on freq 923300000 Hz at DR 8
22:20:30.043 -> 13566s845:IRQ_RX_TX_TIMEOUT
22:20:30.049 -> 13566s846:MAC rxTimeOut
22:20:30.059 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=17, Channel=11
22:35:08.096 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
22:35:08.103 -> 
22:35:08.112 -> [PIMA] Uplink routine
22:35:08.121 -> [PIMA] pima_read_cycle: start (burstMax=60)
22:35:08.131 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:35:09.552 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:11.022 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:12.491 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:13.962 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:15.384 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:15.896 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:35:15.905 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:35:15.914 -> [PIMA] pima_read_cycle: attempt 1 -> fail
22:35:15.922 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:35:17.345 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:18.816 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:20.288 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:21.759 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:23.230 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:35:23.693 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:35:23.702 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:35:23.711 -> [PIMA] pima_read_cycle: attempt 2 -> fail
22:35:23.772 -> [PIMA] pima_read_cycle: overall timeout reached
22:35:23.774 -> [PIMA] pima_read_cycle: no packet captured
22:35:23.784 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
22:35:23.794 -> 14460s653:TX on freq 917800000 Hz at DR 5
22:35:23.854 -> 14460s791:MAC txDone
22:35:28.805 -> 14465s765:RX_1 on freq 926300000 Hz at DR 13
22:35:28.862 -> 14465s806:IRQ_RX_TX_TIMEOUT
22:35:28.869 -> 14465s806:MAC rxTimeOut
22:35:29.839 -> 14466s780:RX_2 on freq 923300000 Hz at DR 8
22:35:29.896 -> 14466s845:IRQ_RX_TX_TIMEOUT
22:35:29.902 -> 14466s846:MAC rxTimeOut
22:35:29.910 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=18, Channel=13
22:50:07.915 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
22:50:07.925 -> 
22:50:07.934 -> [PIMA] Uplink routine
22:50:07.994 -> [PIMA] pima_read_cycle: start (burstMax=60)
22:50:08.001 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:50:09.423 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:10.844 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:12.314 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:13.783 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:15.253 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:15.764 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:50:15.770 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:50:15.779 -> [PIMA] pima_read_cycle: attempt 1 -> fail
22:50:15.790 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
22:50:17.213 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:18.684 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:20.152 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:21.622 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:23.091 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
22:50:23.551 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
22:50:23.557 -> [PIMA] Base frame 0x02 search timeout (no base found)
22:50:23.567 -> [PIMA] pima_read_cycle: attempt 2 -> fail
22:50:23.578 -> [PIMA] pima_read_cycle: overall timeout reached
22:50:23.587 -> [PIMA] pima_read_cycle: no packet captured
22:50:23.648 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
22:50:23.653 -> 15360s653:TX on freq 917000000 Hz at DR 5
22:50:23.712 -> 15360s791:MAC txDone
22:50:28.664 -> 15365s765:RX_1 on freq 923900000 Hz at DR 13
22:50:28.723 -> 15365s806:IRQ_RX_TX_TIMEOUT
22:50:28.730 -> 15365s806:MAC rxTimeOut
22:50:29.699 -> 15366s780:RX_2 on freq 923300000 Hz at DR 8
22:50:29.755 -> 15366s845:IRQ_RX_TX_TIMEOUT
22:50:29.761 -> 15366s846:MAC rxTimeOut
22:50:29.770 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=19, Channel=9
23:05:07.776 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
23:05:07.784 -> 
23:05:07.793 -> [PIMA] Uplink routine
23:05:07.803 -> [PIMA] pima_read_cycle: start (burstMax=60)
23:05:07.809 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:05:09.233 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:10.702 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:12.172 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:13.643 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:15.115 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:15.577 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:05:15.582 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:05:15.643 -> [PIMA] pima_read_cycle: attempt 1 -> fail
23:05:15.649 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:05:17.072 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:18.540 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:20.012 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:21.433 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:22.903 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:05:23.418 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:05:23.423 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:05:23.431 -> [PIMA] pima_read_cycle: attempt 2 -> fail
23:05:23.442 -> [PIMA] pima_read_cycle: overall timeout reached
23:05:23.450 -> [PIMA] pima_read_cycle: no packet captured
23:05:23.462 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
23:05:23.471 -> 16260s653:TX on freq 916800000 Hz at DR 5
23:05:23.531 -> 16260s791:MAC txDone
23:05:28.530 -> 16265s765:RX_1 on freq 923300000 Hz at DR 13
23:05:28.588 -> 16265s806:IRQ_RX_TX_TIMEOUT
23:05:28.594 -> 16265s806:MAC rxTimeOut
23:05:29.514 -> 16266s780:RX_2 on freq 923300000 Hz at DR 8
23:05:29.624 -> 16266s845:IRQ_RX_TX_TIMEOUT
23:05:29.627 -> 16266s846:MAC rxTimeOut
23:05:29.639 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=20, Channel=8
23:20:07.635 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
23:20:07.641 -> 
23:20:07.651 -> [PIMA] Uplink routine
23:20:07.660 -> [PIMA] pima_read_cycle: start (burstMax=60)
23:20:07.670 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:20:09.092 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:10.562 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:12.035 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:13.506 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:14.976 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:15.437 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:20:15.442 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:20:15.454 -> [PIMA] pima_read_cycle: attempt 1 -> fail
23:20:15.465 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:20:16.886 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:18.359 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:19.829 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:21.300 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:22.770 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:20:23.232 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:20:23.289 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:20:23.297 -> [PIMA] pima_read_cycle: attempt 2 -> fail
23:20:23.306 -> [PIMA] pima_read_cycle: overall timeout reached
23:20:23.316 -> [PIMA] pima_read_cycle: no packet captured
23:20:23.327 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
23:20:23.336 -> 17160s653:TX on freq 917200000 Hz at DR 5
23:20:23.395 -> 17160s791:MAC txDone
23:20:28.396 -> 17165s765:RX_1 on freq 924500000 Hz at DR 13
23:20:28.403 -> 17165s806:IRQ_RX_TX_TIMEOUT
23:20:28.412 -> 17165s806:MAC rxTimeOut
23:20:29.380 -> 17166s780:RX_2 on freq 923300000 Hz at DR 8
23:20:29.438 -> 17166s845:IRQ_RX_TX_TIMEOUT
23:20:29.444 -> 17166s846:MAC rxTimeOut
23:20:29.453 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=21, Channel=10
23:35:07.481 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
23:35:07.487 -> 
23:35:07.492 -> [PIMA] Uplink routine
23:35:07.501 -> [PIMA] pima_read_cycle: start (burstMax=60)
23:35:07.508 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:35:08.931 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:10.401 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:11.870 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:13.342 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:14.810 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:15.271 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:35:15.332 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:35:15.339 -> [PIMA] pima_read_cycle: attempt 1 -> fail
23:35:15.348 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:35:16.771 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:18.242 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:19.662 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:21.130 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:22.602 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:35:23.114 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:35:23.121 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:35:23.129 -> [PIMA] pima_read_cycle: attempt 2 -> fail
23:35:23.138 -> [PIMA] pima_read_cycle: overall timeout reached
23:35:23.146 -> [PIMA] pima_read_cycle: no packet captured
23:35:23.157 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
23:35:23.166 -> 18060s653:TX on freq 918000000 Hz at DR 5
23:35:23.226 -> 18060s791:MAC txDone
23:35:28.231 -> 18065s765:RX_1 on freq 926900000 Hz at DR 13
23:35:28.290 -> 18065s806:IRQ_RX_TX_TIMEOUT
23:35:28.292 -> 18065s806:MAC rxTimeOut
23:35:29.259 -> 18066s780:RX_2 on freq 923300000 Hz at DR 8
23:35:29.317 -> 18066s845:IRQ_RX_TX_TIMEOUT
23:35:29.324 -> 18066s846:MAC rxTimeOut
23:35:29.333 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=22, Channel=14
23:50:07.354 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
23:50:07.360 -> 
23:50:07.371 -> [PIMA] Uplink routine
23:50:07.379 -> [PIMA] pima_read_cycle: start (burstMax=60)
23:50:07.389 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:50:08.811 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:10.280 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:11.700 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:13.168 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:14.635 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:15.146 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:50:15.154 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:50:15.164 -> [PIMA] pima_read_cycle: attempt 1 -> fail
23:50:15.173 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
23:50:16.594 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:18.064 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:19.534 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:21.003 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:22.472 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
23:50:22.934 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
23:50:22.941 -> [PIMA] Base frame 0x02 search timeout (no base found)
23:50:23.000 -> [PIMA] pima_read_cycle: attempt 2 -> fail
23:50:23.006 -> [PIMA] pima_read_cycle: overall timeout reached
23:50:23.015 -> [PIMA] pima_read_cycle: no packet captured
23:50:23.025 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
23:50:23.034 -> 18960s653:TX on freq 918200000 Hz at DR 5
23:50:23.094 -> 18960s791:MAC txDone
23:50:28.089 -> 18965s765:RX_1 on freq 927500000 Hz at DR 13
23:50:28.094 -> 18965s806:IRQ_RX_TX_TIMEOUT
23:50:28.105 -> 18965s806:MAC rxTimeOut
23:50:29.074 -> 18966s780:RX_2 on freq 923300000 Hz at DR 8
23:50:29.131 -> 18966s845:IRQ_RX_TX_TIMEOUT
23:50:29.138 -> 18966s846:MAC rxTimeOut
23:50:29.148 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=23, Channel=15
00:05:07.180 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
00:05:07.186 -> 
00:05:07.195 -> [PIMA] Uplink routine
00:05:07.205 -> [PIMA] pima_read_cycle: start (burstMax=60)
00:05:07.213 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:05:08.634 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:10.103 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:11.570 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:13.036 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:14.505 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:14.967 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:05:15.024 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:05:15.032 -> [PIMA] pima_read_cycle: attempt 1 -> fail
00:05:15.042 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:05:16.466 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:17.940 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:19.360 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:20.831 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:22.299 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:05:22.813 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:05:22.821 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:05:22.832 -> [PIMA] pima_read_cycle: attempt 2 -> fail
00:05:22.841 -> [PIMA] pima_read_cycle: overall timeout reached
00:05:22.846 -> [PIMA] pima_read_cycle: no packet captured
00:05:22.857 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
00:05:22.865 -> 19860s653:TX on freq 917600000 Hz at DR 5
00:05:22.922 -> 19860s791:MAC txDone
00:05:27.921 -> 19865s765:RX_1 on freq 925700000 Hz at DR 13
00:05:27.980 -> 19865s806:IRQ_RX_TX_TIMEOUT
00:05:27.986 -> 19865s806:MAC rxTimeOut
00:05:28.948 -> 19866s780:RX_2 on freq 923300000 Hz at DR 8
00:05:29.007 -> 19866s845:IRQ_RX_TX_TIMEOUT
00:05:29.011 -> 19866s846:MAC rxTimeOut
00:05:29.021 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=24, Channel=12
00:20:07.042 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
00:20:07.048 -> 
00:20:07.058 -> [PIMA] Uplink routine
00:20:07.068 -> [PIMA] pima_read_cycle: start (burstMax=60)
00:20:07.074 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:20:08.496 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:09.968 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:11.440 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:12.861 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:14.335 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:14.848 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:20:14.854 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:20:14.863 -> [PIMA] pima_read_cycle: attempt 1 -> fail
00:20:14.873 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:20:16.294 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:17.768 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:19.238 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:20.711 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:22.182 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:20:22.645 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:20:22.650 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:20:22.661 -> [PIMA] pima_read_cycle: attempt 2 -> fail
00:20:22.669 -> [PIMA] pima_read_cycle: overall timeout reached
00:20:22.678 -> [PIMA] pima_read_cycle: no packet captured
00:20:22.739 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
00:20:22.746 -> 20760s653:TX on freq 918200000 Hz at DR 5
00:20:22.802 -> 20760s791:MAC txDone
00:20:27.755 -> 20765s765:RX_1 on freq 927500000 Hz at DR 13
00:20:27.813 -> 20765s806:IRQ_RX_TX_TIMEOUT
00:20:27.821 -> 20765s806:MAC rxTimeOut
00:20:28.789 -> 20766s780:RX_2 on freq 923300000 Hz at DR 8
00:20:28.849 -> 20766s845:IRQ_RX_TX_TIMEOUT
00:20:28.856 -> 20766s846:MAC rxTimeOut
00:20:28.866 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=25, Channel=15
00:35:06.867 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
00:35:06.875 -> 
00:35:06.886 -> [PIMA] Uplink routine
00:35:06.895 -> [PIMA] pima_read_cycle: start (burstMax=60)
00:35:06.907 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:35:08.330 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:09.800 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:11.269 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:12.741 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:14.213 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:14.676 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:35:14.683 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:35:14.692 -> [PIMA] pima_read_cycle: attempt 1 -> fail
00:35:14.702 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:35:16.174 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:17.594 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:19.066 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:20.532 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:22.005 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:35:22.517 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:35:22.529 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:35:22.537 -> [PIMA] pima_read_cycle: attempt 2 -> fail
00:35:22.546 -> [PIMA] pima_read_cycle: overall timeout reached
00:35:22.556 -> [PIMA] pima_read_cycle: no packet captured
00:35:22.565 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
00:35:22.574 -> 21660s653:TX on freq 917200000 Hz at DR 5
00:35:22.633 -> 21660s791:MAC txDone
00:35:27.637 -> 21665s765:RX_1 on freq 924500000 Hz at DR 13
00:35:27.648 -> 21665s806:IRQ_RX_TX_TIMEOUT
00:35:27.657 -> 21665s806:MAC rxTimeOut
00:35:28.623 -> 21666s780:RX_2 on freq 923300000 Hz at DR 8
00:35:28.680 -> 21666s845:IRQ_RX_TX_TIMEOUT
00:35:28.691 -> 21666s846:MAC rxTimeOut
00:35:28.700 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=26, Channel=10
00:50:06.698 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
00:50:06.704 -> 
00:50:06.764 -> [PIMA] Uplink routine
00:50:06.774 -> [PIMA] pima_read_cycle: start (burstMax=60)
00:50:06.783 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:50:08.205 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:09.626 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:11.096 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:12.565 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:14.035 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:14.547 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:50:14.557 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:50:14.567 -> [PIMA] pima_read_cycle: attempt 1 -> fail
00:50:14.577 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
00:50:15.999 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:17.469 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:18.938 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:20.406 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:21.874 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
00:50:22.335 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
00:50:22.344 -> [PIMA] Base frame 0x02 search timeout (no base found)
00:50:22.353 -> [PIMA] pima_read_cycle: attempt 2 -> fail
00:50:22.364 -> [PIMA] pima_read_cycle: overall timeout reached
00:50:22.424 -> [PIMA] pima_read_cycle: no packet captured
00:50:22.430 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
00:50:22.439 -> 22560s653:TX on freq 916800000 Hz at DR 5
00:50:22.500 -> 22560s791:MAC txDone
00:50:27.447 -> 22565s765:RX_1 on freq 923300000 Hz at DR 13
00:50:27.499 -> 22565s806:IRQ_RX_TX_TIMEOUT
00:50:27.508 -> 22565s806:MAC rxTimeOut
00:50:28.476 -> 22566s780:RX_2 on freq 923300000 Hz at DR 8
00:50:28.533 -> 22566s845:IRQ_RX_TX_TIMEOUT
00:50:28.539 -> 22566s846:MAC rxTimeOut
00:50:28.548 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=27, Channel=8
01:05:06.568 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
01:05:06.576 -> 
01:05:06.586 -> [PIMA] Uplink routine
01:05:06.597 -> [PIMA] pima_read_cycle: start (burstMax=60)
01:05:06.602 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:05:08.026 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:09.496 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:10.966 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:12.434 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:13.903 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:14.369 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:05:14.378 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:05:14.388 -> [PIMA] pima_read_cycle: attempt 1 -> fail
01:05:14.448 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:05:15.868 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:17.288 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:18.760 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:20.233 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:21.705 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:05:22.169 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:05:22.229 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:05:22.237 -> [PIMA] pima_read_cycle: attempt 2 -> fail
01:05:22.246 -> [PIMA] pima_read_cycle: overall timeout reached
01:05:22.255 -> [PIMA] pima_read_cycle: no packet captured
01:05:22.265 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
01:05:22.275 -> 23460s653:TX on freq 917400000 Hz at DR 5
01:05:22.334 -> 23460s791:MAC txDone
01:05:27.286 -> 23465s765:RX_1 on freq 925100000 Hz at DR 13
01:05:27.343 -> 23465s806:IRQ_RX_TX_TIMEOUT
01:05:27.351 -> 23465s806:MAC rxTimeOut
01:05:28.314 -> 23466s780:RX_2 on freq 923300000 Hz at DR 8
01:05:28.373 -> 23466s845:IRQ_RX_TX_TIMEOUT
01:05:28.378 -> 23466s846:MAC rxTimeOut
01:05:28.388 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=28, Channel=11
01:20:06.406 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
01:20:06.415 -> 
01:20:06.425 -> [PIMA] Uplink routine
01:20:06.434 -> [PIMA] pima_read_cycle: start (burstMax=60)
01:20:06.439 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:20:07.861 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:09.329 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:10.801 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:12.271 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:13.741 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:14.203 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:20:14.260 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:20:14.267 -> [PIMA] pima_read_cycle: attempt 1 -> fail
01:20:14.276 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:20:15.700 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:17.168 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:18.638 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:20.108 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:21.576 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:20:22.037 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:20:22.043 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:20:22.052 -> [PIMA] pima_read_cycle: attempt 2 -> fail
01:20:22.062 -> [PIMA] pima_read_cycle: overall timeout reached
01:20:22.072 -> [PIMA] pima_read_cycle: no packet captured
01:20:22.128 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
01:20:22.133 -> 24360s653:TX on freq 918000000 Hz at DR 5
01:20:22.194 -> 24360s791:MAC txDone
01:20:27.146 -> 24365s765:RX_1 on freq 926900000 Hz at DR 13
01:20:27.205 -> 24365s806:IRQ_RX_TX_TIMEOUT
01:20:27.213 -> 24365s806:MAC rxTimeOut
01:20:28.181 -> 24366s780:RX_2 on freq 923300000 Hz at DR 8
01:20:28.240 -> 24366s845:IRQ_RX_TX_TIMEOUT
01:20:28.247 -> 24366s846:MAC rxTimeOut
01:20:28.255 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=29, Channel=14
01:35:06.278 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
01:35:06.284 -> 
01:35:06.294 -> [PIMA] Uplink routine
01:35:06.303 -> [PIMA] pima_read_cycle: start (burstMax=60)
01:35:06.313 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:35:07.731 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:09.204 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:10.676 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:12.143 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:13.563 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:14.073 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:35:14.080 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:35:14.089 -> [PIMA] pima_read_cycle: attempt 1 -> fail
01:35:14.097 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:35:15.518 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:16.988 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:18.461 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:19.932 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:21.403 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:35:21.869 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:35:21.876 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:35:21.935 -> [PIMA] pima_read_cycle: attempt 2 -> fail
01:35:21.944 -> [PIMA] pima_read_cycle: overall timeout reached
01:35:21.954 -> [PIMA] pima_read_cycle: no packet captured
01:35:21.964 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
01:35:21.972 -> 25260s653:TX on freq 917000000 Hz at DR 5
01:35:22.030 -> 25260s791:MAC txDone
01:35:26.979 -> 25265s765:RX_1 on freq 923900000 Hz at DR 13
01:35:27.038 -> 25265s806:IRQ_RX_TX_TIMEOUT
01:35:27.046 -> 25265s806:MAC rxTimeOut
01:35:28.013 -> 25266s780:RX_2 on freq 923300000 Hz at DR 8
01:35:28.072 -> 25266s845:IRQ_RX_TX_TIMEOUT
01:35:28.079 -> 25266s846:MAC rxTimeOut
01:35:28.090 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=30, Channel=9
01:50:06.136 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
01:50:06.143 -> 
01:50:06.151 -> [PIMA] Uplink routine
01:50:06.162 -> [PIMA] pima_read_cycle: start (burstMax=60)
01:50:06.171 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:50:07.592 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:09.061 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:10.532 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:11.949 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:13.419 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:13.931 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:50:13.938 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:50:13.947 -> [PIMA] pima_read_cycle: attempt 1 -> fail
01:50:13.956 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
01:50:15.376 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:16.849 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:18.316 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:19.787 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:21.258 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
01:50:21.719 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
01:50:21.725 -> [PIMA] Base frame 0x02 search timeout (no base found)
01:50:21.735 -> [PIMA] pima_read_cycle: attempt 2 -> fail
01:50:21.796 -> [PIMA] pima_read_cycle: overall timeout reached
01:50:21.803 -> [PIMA] pima_read_cycle: no packet captured
01:50:21.814 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
01:50:21.822 -> 26160s653:TX on freq 917800000 Hz at DR 5
01:50:21.884 -> 26160s791:MAC txDone
01:50:26.836 -> 26165s765:RX_1 on freq 926300000 Hz at DR 13
01:50:26.892 -> 26165s806:IRQ_RX_TX_TIMEOUT
01:50:26.899 -> 26165s806:MAC rxTimeOut
01:50:27.869 -> 26166s780:RX_2 on freq 923300000 Hz at DR 8
01:50:27.928 -> 26166s846:IRQ_RX_TX_TIMEOUT
01:50:27.935 -> 26166s846:MAC rxTimeOut
01:50:27.945 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=31, Channel=13
02:05:05.973 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
02:05:05.984 -> 
02:05:05.993 -> [PIMA] Uplink routine
02:05:06.002 -> [PIMA] pima_read_cycle: start (burstMax=60)
02:05:06.011 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:05:07.435 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:08.905 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:10.377 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:11.796 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:13.264 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:13.776 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:05:13.783 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:05:13.793 -> [PIMA] pima_read_cycle: attempt 1 -> fail
02:05:13.802 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:05:15.224 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:16.693 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:18.163 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:19.637 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:21.108 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:05:21.571 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:05:21.582 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:05:21.593 -> [PIMA] pima_read_cycle: attempt 2 -> fail
02:05:21.652 -> [PIMA] pima_read_cycle: overall timeout reached
02:05:21.658 -> [PIMA] pima_read_cycle: no packet captured
02:05:21.669 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
02:05:21.675 -> 27060s653:TX on freq 917600000 Hz at DR 5
02:05:21.736 -> 27060s791:MAC txDone
02:05:26.687 -> 27065s765:RX_1 on freq 925700000 Hz at DR 13
02:05:26.747 -> 27065s806:IRQ_RX_TX_TIMEOUT
02:05:26.751 -> 27065s806:MAC rxTimeOut
02:05:27.723 -> 27066s780:RX_2 on freq 923300000 Hz at DR 8
02:05:27.779 -> 27066s846:IRQ_RX_TX_TIMEOUT
02:05:27.786 -> 27066s846:MAC rxTimeOut
02:05:27.796 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=32, Channel=12
02:20:05.790 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
02:20:05.798 -> 
02:20:05.809 -> [PIMA] Uplink routine
02:20:05.819 -> [PIMA] pima_read_cycle: start (burstMax=60)
02:20:05.880 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:20:07.249 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:08.718 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:10.187 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:11.660 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:13.134 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:13.594 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:20:13.652 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:20:13.658 -> [PIMA] pima_read_cycle: attempt 1 -> fail
02:20:13.667 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:20:15.088 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:16.558 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:18.026 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:19.495 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:20.966 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:20:21.428 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:20:21.435 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:20:21.443 -> [PIMA] pima_read_cycle: attempt 2 -> fail
02:20:21.454 -> [PIMA] pima_read_cycle: overall timeout reached
02:20:21.462 -> [PIMA] pima_read_cycle: no packet captured
02:20:21.472 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
02:20:21.530 -> 27960s653:TX on freq 917200000 Hz at DR 5
02:20:21.588 -> 27960s791:MAC txDone
02:20:26.539 -> 27965s765:RX_1 on freq 924500000 Hz at DR 13
02:20:26.597 -> 27965s806:IRQ_RX_TX_TIMEOUT
02:20:26.602 -> 27965s806:MAC rxTimeOut
02:20:27.573 -> 27966s780:RX_2 on freq 923300000 Hz at DR 8
02:20:27.634 -> 27966s845:IRQ_RX_TX_TIMEOUT
02:20:27.642 -> 27966s846:MAC rxTimeOut
02:20:27.652 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=33, Channel=10
02:35:05.654 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
02:35:05.664 -> 
02:35:05.672 -> [PIMA] Uplink routine
02:35:05.678 -> [PIMA] pima_read_cycle: start (burstMax=60)
02:35:05.689 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:35:07.112 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:08.583 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:10.054 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:11.518 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:12.987 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:13.452 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:35:13.459 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:35:13.469 -> [PIMA] pima_read_cycle: attempt 1 -> fail
02:35:13.528 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:35:14.949 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:16.419 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:17.838 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:19.309 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:20.780 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:35:21.288 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:35:21.296 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:35:21.305 -> [PIMA] pima_read_cycle: attempt 2 -> fail
02:35:21.315 -> [PIMA] pima_read_cycle: overall timeout reached
02:35:21.324 -> [PIMA] pima_read_cycle: no packet captured
02:35:21.333 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
02:35:21.343 -> 28860s652:TX on freq 918200000 Hz at DR 5
02:35:21.403 -> 28860s791:MAC txDone
02:35:26.405 -> 28865s764:RX_1 on freq 927500000 Hz at DR 13
02:35:26.465 -> 28865s805:IRQ_RX_TX_TIMEOUT
02:35:26.471 -> 28865s805:MAC rxTimeOut
02:35:27.389 -> 28866s779:RX_2 on freq 923300000 Hz at DR 8
02:35:27.450 -> 28866s845:IRQ_RX_TX_TIMEOUT
02:35:27.457 -> 28866s845:MAC rxTimeOut
02:35:27.517 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=34, Channel=15
02:50:05.517 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
02:50:05.523 -> 
02:50:05.533 -> [PIMA] Uplink routine
02:50:05.542 -> [PIMA] pima_read_cycle: start (burstMax=60)
02:50:05.552 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:50:06.977 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:08.448 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:09.918 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:11.339 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:12.810 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:13.322 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:50:13.328 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:50:13.337 -> [PIMA] pima_read_cycle: attempt 1 -> fail
02:50:13.348 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
02:50:14.771 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:16.237 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:17.705 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:19.173 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:20.642 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
02:50:21.104 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
02:50:21.110 -> [PIMA] Base frame 0x02 search timeout (no base found)
02:50:21.170 -> [PIMA] pima_read_cycle: attempt 2 -> fail
02:50:21.176 -> [PIMA] pima_read_cycle: overall timeout reached
02:50:21.186 -> [PIMA] pima_read_cycle: no packet captured
02:50:21.196 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
02:50:21.207 -> 29760s653:TX on freq 918000000 Hz at DR 5
02:50:21.267 -> 29760s791:MAC txDone
02:50:26.215 -> 29765s765:RX_1 on freq 926900000 Hz at DR 13
02:50:26.273 -> 29765s806:IRQ_RX_TX_TIMEOUT
02:50:26.280 -> 29765s806:MAC rxTimeOut
02:50:27.249 -> 29766s780:RX_2 on freq 923300000 Hz at DR 8
02:50:27.307 -> 29766s846:IRQ_RX_TX_TIMEOUT
02:50:27.313 -> 29766s846:MAC rxTimeOut
02:50:27.322 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=35, Channel=14
03:05:05.349 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
03:05:05.355 -> 
03:05:05.363 -> [PIMA] Uplink routine
03:05:05.370 -> [PIMA] pima_read_cycle: start (burstMax=60)
03:05:05.379 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:05:06.801 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:08.270 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:09.741 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:11.213 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:12.681 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:13.138 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:05:13.196 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:05:13.204 -> [PIMA] pima_read_cycle: attempt 1 -> fail
03:05:13.213 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:05:14.634 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:16.104 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:17.573 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:18.996 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:20.467 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:05:20.980 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:05:20.986 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:05:20.994 -> [PIMA] pima_read_cycle: attempt 2 -> fail
03:05:21.003 -> [PIMA] pima_read_cycle: overall timeout reached
03:05:21.011 -> [PIMA] pima_read_cycle: no packet captured
03:05:21.022 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
03:05:21.030 -> 30660s653:TX on freq 916800000 Hz at DR 5
03:05:21.092 -> 30660s791:MAC txDone
03:05:26.093 -> 30665s765:RX_1 on freq 923300000 Hz at DR 13
03:05:26.151 -> 30665s806:IRQ_RX_TX_TIMEOUT
03:05:26.158 -> 30665s806:MAC rxTimeOut
03:05:27.076 -> 30666s780:RX_2 on freq 923300000 Hz at DR 8
03:05:27.187 -> 30666s846:IRQ_RX_TX_TIMEOUT
03:05:27.195 -> 30666s846:MAC rxTimeOut
03:05:27.206 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=36, Channel=8
03:20:05.191 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
03:20:05.198 -> 
03:20:05.207 -> [PIMA] Uplink routine
03:20:05.217 -> [PIMA] pima_read_cycle: start (burstMax=60)
03:20:05.227 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:20:06.650 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:08.119 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:09.588 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:11.060 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:12.534 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:12.994 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:20:13.001 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:20:13.009 -> [PIMA] pima_read_cycle: attempt 1 -> fail
03:20:13.065 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:20:14.484 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:15.952 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:17.375 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:18.845 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:20.315 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:20:20.828 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:20:20.834 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:20:20.845 -> [PIMA] pima_read_cycle: attempt 2 -> fail
03:20:20.855 -> [PIMA] pima_read_cycle: overall timeout reached
03:20:20.864 -> [PIMA] pima_read_cycle: no packet captured
03:20:20.874 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
03:20:20.884 -> 31560s653:TX on freq 917000000 Hz at DR 5
03:20:20.945 -> 31560s791:MAC txDone
03:20:25.950 -> 31565s765:RX_1 on freq 923900000 Hz at DR 13
03:20:25.957 -> 31565s806:IRQ_RX_TX_TIMEOUT
03:20:25.967 -> 31565s806:MAC rxTimeOut
03:20:26.934 -> 31566s780:RX_2 on freq 923300000 Hz at DR 8
03:20:26.992 -> 31566s846:IRQ_RX_TX_TIMEOUT
03:20:26.997 -> 31566s846:MAC rxTimeOut
03:20:27.054 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=37, Channel=9
03:35:05.066 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
03:35:05.074 -> 
03:35:05.083 -> [PIMA] Uplink routine
03:35:05.093 -> [PIMA] pima_read_cycle: start (burstMax=60)
03:35:05.102 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:35:06.524 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:07.995 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:09.415 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:10.884 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:12.354 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:12.864 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:35:12.870 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:35:12.878 -> [PIMA] pima_read_cycle: attempt 1 -> fail
03:35:12.888 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:35:14.307 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:15.777 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:17.241 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:18.712 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:20.183 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:35:20.644 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:35:20.652 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:35:20.712 -> [PIMA] pima_read_cycle: attempt 2 -> fail
03:35:20.719 -> [PIMA] pima_read_cycle: overall timeout reached
03:35:20.728 -> [PIMA] pima_read_cycle: no packet captured
03:35:20.738 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
03:35:20.749 -> 32460s653:TX on freq 917800000 Hz at DR 5
03:35:20.808 -> 32460s791:MAC txDone
03:35:25.759 -> 32465s765:RX_1 on freq 926300000 Hz at DR 13
03:35:25.820 -> 32465s806:IRQ_RX_TX_TIMEOUT
03:35:25.829 -> 32465s806:MAC rxTimeOut
03:35:26.796 -> 32466s780:RX_2 on freq 923300000 Hz at DR 8
03:35:26.855 -> 32466s846:IRQ_RX_TX_TIMEOUT
03:35:26.861 -> 32466s846:MAC rxTimeOut
03:35:26.871 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=38, Channel=13
03:50:04.865 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
03:50:04.873 -> 
03:50:04.932 -> [PIMA] Uplink routine
03:50:04.939 -> [PIMA] pima_read_cycle: start (burstMax=60)
03:50:04.949 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:50:06.371 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:07.840 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:09.258 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:10.728 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:12.197 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:12.709 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:50:12.716 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:50:12.726 -> [PIMA] pima_read_cycle: attempt 1 -> fail
03:50:12.734 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
03:50:14.157 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:15.626 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:17.095 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:18.564 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:20.034 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
03:50:20.495 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
03:50:20.501 -> [PIMA] Base frame 0x02 search timeout (no base found)
03:50:20.510 -> [PIMA] pima_read_cycle: attempt 2 -> fail
03:50:20.571 -> [PIMA] pima_read_cycle: overall timeout reached
03:50:20.580 -> [PIMA] pima_read_cycle: no packet captured
03:50:20.588 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
03:50:20.598 -> 33360s653:TX on freq 917400000 Hz at DR 5
03:50:20.658 -> 33360s791:MAC txDone
03:50:25.607 -> 33365s765:RX_1 on freq 925100000 Hz at DR 13
03:50:25.665 -> 33365s806:IRQ_RX_TX_TIMEOUT
03:50:25.671 -> 33365s806:MAC rxTimeOut
03:50:26.639 -> 33366s780:RX_2 on freq 923300000 Hz at DR 8
03:50:26.696 -> 33366s846:IRQ_RX_TX_TIMEOUT
03:50:26.702 -> 33366s846:MAC rxTimeOut
03:50:26.710 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=39, Channel=11
04:05:04.749 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
04:05:04.759 -> 
04:05:04.767 -> [PIMA] Uplink routine
04:05:04.774 -> [PIMA] pima_read_cycle: start (burstMax=60)
04:05:04.783 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:05:06.206 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:07.677 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:09.149 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:10.574 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:12.042 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:12.552 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:05:12.558 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:05:12.569 -> [PIMA] pima_read_cycle: attempt 1 -> fail
04:05:12.580 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:05:14.001 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:15.474 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:16.947 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:18.420 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:19.892 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:05:20.356 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:05:20.363 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:05:20.373 -> [PIMA] pima_read_cycle: attempt 2 -> fail
04:05:20.383 -> [PIMA] pima_read_cycle: overall timeout reached
04:05:20.392 -> [PIMA] pima_read_cycle: no packet captured
04:05:20.401 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
04:05:20.462 -> 34260s653:TX on freq 917800000 Hz at DR 5
04:05:20.523 -> 34260s791:MAC txDone
04:05:25.476 -> 34265s765:RX_1 on freq 926300000 Hz at DR 13
04:05:25.534 -> 34265s806:IRQ_RX_TX_TIMEOUT
04:05:25.539 -> 34265s806:MAC rxTimeOut
04:05:26.509 -> 34266s780:RX_2 on freq 923300000 Hz at DR 8
04:05:26.567 -> 34266s846:IRQ_RX_TX_TIMEOUT
04:05:26.573 -> 34266s846:MAC rxTimeOut
04:05:26.583 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=40, Channel=13
04:20:04.581 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
04:20:04.589 -> 
04:20:04.598 -> [PIMA] Uplink routine
04:20:04.607 -> [PIMA] pima_read_cycle: start (burstMax=60)
04:20:04.617 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:20:06.038 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:07.507 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:08.978 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:10.448 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:11.919 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:12.379 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:20:12.389 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:20:12.398 -> [PIMA] pima_read_cycle: attempt 1 -> fail
04:20:12.458 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:20:13.876 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:15.346 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:16.764 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:18.232 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:19.703 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:20:20.213 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:20:20.219 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:20:20.229 -> [PIMA] pima_read_cycle: attempt 2 -> fail
04:20:20.238 -> [PIMA] pima_read_cycle: overall timeout reached
04:20:20.247 -> [PIMA] pima_read_cycle: no packet captured
04:20:20.253 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
04:20:20.262 -> 35160s653:TX on freq 917600000 Hz at DR 5
04:20:20.323 -> 35160s791:MAC txDone
04:20:25.327 -> 35165s765:RX_1 on freq 925700000 Hz at DR 13
04:20:25.387 -> 35165s806:IRQ_RX_TX_TIMEOUT
04:20:25.394 -> 35165s806:MAC rxTimeOut
04:20:26.311 -> 35166s780:RX_2 on freq 923300000 Hz at DR 8
04:20:26.419 -> 35166s846:IRQ_RX_TX_TIMEOUT
04:20:26.425 -> 35166s846:MAC rxTimeOut
04:20:26.435 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=41, Channel=12
04:35:04.441 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
04:35:04.447 -> 
04:35:04.457 -> [PIMA] Uplink routine
04:35:04.465 -> [PIMA] pima_read_cycle: start (burstMax=60)
04:35:04.474 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:35:05.896 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:07.370 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:08.838 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:10.309 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:11.729 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:12.239 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:35:12.245 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:35:12.254 -> [PIMA] pima_read_cycle: attempt 1 -> fail
04:35:12.263 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:35:13.685 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:15.154 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:16.625 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:18.096 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:19.564 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:35:20.026 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:35:20.083 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:35:20.091 -> [PIMA] pima_read_cycle: attempt 2 -> fail
04:35:20.097 -> [PIMA] pima_read_cycle: overall timeout reached
04:35:20.107 -> [PIMA] pima_read_cycle: no packet captured
04:35:20.116 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
04:35:20.126 -> 36060s652:TX on freq 916800000 Hz at DR 5
04:35:20.187 -> 36060s791:MAC txDone
04:35:25.188 -> 36065s764:RX_1 on freq 923300000 Hz at DR 13
04:35:25.193 -> 36065s805:IRQ_RX_TX_TIMEOUT
04:35:25.203 -> 36065s805:MAC rxTimeOut
04:35:26.168 -> 36066s779:RX_2 on freq 923300000 Hz at DR 8
04:35:26.225 -> 36066s845:IRQ_RX_TX_TIMEOUT
04:35:26.231 -> 36066s845:MAC rxTimeOut
04:35:26.242 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=42, Channel=8
04:50:04.275 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
04:50:04.282 -> 
04:50:04.292 -> [PIMA] Uplink routine
04:50:04.301 -> [PIMA] pima_read_cycle: start (burstMax=60)
04:50:04.311 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:50:05.734 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:07.205 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:08.678 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:10.149 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:11.621 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:12.083 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:50:12.092 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:50:12.101 -> [PIMA] pima_read_cycle: attempt 1 -> fail
04:50:12.110 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
04:50:13.534 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:15.007 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:16.478 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:17.947 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:19.416 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
04:50:19.877 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
04:50:19.886 -> [PIMA] Base frame 0x02 search timeout (no base found)
04:50:19.945 -> [PIMA] pima_read_cycle: attempt 2 -> fail
04:50:19.953 -> [PIMA] pima_read_cycle: overall timeout reached
04:50:19.965 -> [PIMA] pima_read_cycle: no packet captured
04:50:19.975 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
04:50:19.985 -> 36960s653:TX on freq 917400000 Hz at DR 5
04:50:20.044 -> 36960s791:MAC txDone
04:50:24.995 -> 36965s765:RX_1 on freq 925100000 Hz at DR 13
04:50:25.051 -> 36965s806:IRQ_RX_TX_TIMEOUT
04:50:25.057 -> 36965s806:MAC rxTimeOut
04:50:26.025 -> 36966s780:RX_2 on freq 923300000 Hz at DR 8
04:50:26.082 -> 36966s846:IRQ_RX_TX_TIMEOUT
04:50:26.091 -> 36966s846:MAC rxTimeOut
04:50:26.103 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=43, Channel=11
05:05:04.119 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
05:05:04.125 -> 
05:05:04.134 -> [PIMA] Uplink routine
05:05:04.145 -> [PIMA] pima_read_cycle: start (burstMax=60)
05:05:04.154 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:05:05.574 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:07.045 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:08.515 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:09.985 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:11.453 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:11.914 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:05:11.921 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:05:11.929 -> [PIMA] pima_read_cycle: attempt 1 -> fail
05:05:11.986 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:05:13.405 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:14.875 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:16.344 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:17.812 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:19.234 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:05:19.746 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:05:19.754 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:05:19.764 -> [PIMA] pima_read_cycle: attempt 2 -> fail
05:05:19.772 -> [PIMA] pima_read_cycle: overall timeout reached
05:05:19.781 -> [PIMA] pima_read_cycle: no packet captured
05:05:19.790 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
05:05:19.800 -> 37860s653:TX on freq 917000000 Hz at DR 5
05:05:19.861 -> 37860s791:MAC txDone
05:05:24.860 -> 37865s765:RX_1 on freq 923900000 Hz at DR 13
05:05:24.917 -> 37865s806:IRQ_RX_TX_TIMEOUT
05:05:24.925 -> 37865s806:MAC rxTimeOut
05:05:25.894 -> 37866s780:RX_2 on freq 923300000 Hz at DR 8
05:05:25.951 -> 37866s846:IRQ_RX_TX_TIMEOUT
05:05:25.958 -> 37866s846:MAC rxTimeOut
05:05:25.968 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=44, Channel=9
05:20:03.978 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
05:20:03.984 -> 
05:20:03.994 -> [PIMA] Uplink routine
05:20:04.003 -> [PIMA] pima_read_cycle: start (burstMax=60)
05:20:04.012 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:20:05.434 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:06.905 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:08.377 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:09.798 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:11.270 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:11.782 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:20:11.788 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:20:11.798 -> [PIMA] pima_read_cycle: attempt 1 -> fail
05:20:11.808 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:20:13.229 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:14.698 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:16.171 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:17.641 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:19.111 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:20:19.574 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:20:19.580 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:20:19.591 -> [PIMA] pima_read_cycle: attempt 2 -> fail
05:20:19.652 -> [PIMA] pima_read_cycle: overall timeout reached
05:20:19.657 -> [PIMA] pima_read_cycle: no packet captured
05:20:19.666 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
05:20:19.675 -> 38760s653:TX on freq 918200000 Hz at DR 5
05:20:19.735 -> 38760s791:MAC txDone
05:20:24.687 -> 38765s765:RX_1 on freq 927500000 Hz at DR 13
05:20:24.745 -> 38765s806:IRQ_RX_TX_TIMEOUT
05:20:24.750 -> 38765s806:MAC rxTimeOut
05:20:25.717 -> 38766s780:RX_2 on freq 923300000 Hz at DR 8
05:20:25.776 -> 38766s846:IRQ_RX_TX_TIMEOUT
05:20:25.782 -> 38766s846:MAC rxTimeOut
05:20:25.792 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=45, Channel=15
05:35:03.807 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
05:35:03.813 -> 
05:35:03.821 -> [PIMA] Uplink routine
05:35:03.828 -> [PIMA] pima_read_cycle: start (burstMax=60)
05:35:03.837 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:35:05.260 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:06.731 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:08.201 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:09.675 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:11.145 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:11.606 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:35:11.614 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:35:11.624 -> [PIMA] pima_read_cycle: attempt 1 -> fail
05:35:11.683 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:35:13.103 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:14.526 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:15.996 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:17.467 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:18.937 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:35:19.449 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:35:19.458 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:35:19.468 -> [PIMA] pima_read_cycle: attempt 2 -> fail
05:35:19.480 -> [PIMA] pima_read_cycle: overall timeout reached
05:35:19.490 -> [PIMA] pima_read_cycle: no packet captured
05:35:19.495 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
05:35:19.503 -> 39660s653:TX on freq 918000000 Hz at DR 5
05:35:19.563 -> 39660s791:MAC txDone
05:35:24.560 -> 39665s765:RX_1 on freq 926900000 Hz at DR 13
05:35:24.617 -> 39665s806:IRQ_RX_TX_TIMEOUT
05:35:24.623 -> 39665s806:MAC rxTimeOut
05:35:25.541 -> 39666s780:RX_2 on freq 923300000 Hz at DR 8
05:35:25.648 -> 39666s846:IRQ_RX_TX_TIMEOUT
05:35:25.654 -> 39666s846:MAC rxTimeOut
05:35:25.663 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=46, Channel=14
05:50:03.637 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
05:50:03.643 -> 
05:50:03.652 -> [PIMA] Uplink routine
05:50:03.662 -> [PIMA] pima_read_cycle: start (burstMax=60)
05:50:03.718 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:50:05.143 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:06.562 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:08.030 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:09.501 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:10.971 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:11.484 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:50:11.493 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:50:11.501 -> [PIMA] pima_read_cycle: attempt 1 -> fail
05:50:11.511 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
05:50:12.932 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:14.404 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:15.877 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:17.347 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:18.814 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
05:50:19.275 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
05:50:19.282 -> [PIMA] Base frame 0x02 search timeout (no base found)
05:50:19.292 -> [PIMA] pima_read_cycle: attempt 2 -> fail
05:50:19.301 -> [PIMA] pima_read_cycle: overall timeout reached
05:50:19.307 -> [PIMA] pima_read_cycle: no packet captured
05:50:19.317 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
05:50:19.374 -> 40560s653:TX on freq 917200000 Hz at DR 5
05:50:19.431 -> 40560s791:MAC txDone
05:50:24.378 -> 40565s765:RX_1 on freq 924500000 Hz at DR 13
05:50:24.434 -> 40565s806:IRQ_RX_TX_TIMEOUT
05:50:24.441 -> 40565s806:MAC rxTimeOut
05:50:25.407 -> 40566s780:RX_2 on freq 923300000 Hz at DR 8
05:50:25.464 -> 40566s846:IRQ_RX_TX_TIMEOUT
05:50:25.471 -> 40566s846:MAC rxTimeOut
05:50:25.480 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=47, Channel=10
06:05:03.513 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
06:05:03.520 -> 
06:05:03.530 -> [PIMA] Uplink routine
06:05:03.540 -> [PIMA] pima_read_cycle: start (burstMax=60)
06:05:03.549 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:05:04.974 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:06.443 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:07.916 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:09.337 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:10.802 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:11.313 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:05:11.321 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:05:11.329 -> [PIMA] pima_read_cycle: attempt 1 -> fail
06:05:11.337 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:05:12.760 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:14.230 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:15.705 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:17.176 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:18.646 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:05:19.106 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:05:19.113 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:05:19.122 -> [PIMA] pima_read_cycle: attempt 2 -> fail
06:05:19.182 -> [PIMA] pima_read_cycle: overall timeout reached
06:05:19.189 -> [PIMA] pima_read_cycle: no packet captured
06:05:19.197 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
06:05:19.203 -> 41460s653:TX on freq 917800000 Hz at DR 5
06:05:19.264 -> 41460s791:MAC txDone
06:05:24.262 -> 41465s765:RX_1 on freq 926300000 Hz at DR 13
06:05:24.268 -> 41465s806:IRQ_RX_TX_TIMEOUT
06:05:24.278 -> 41465s806:MAC rxTimeOut
06:05:25.242 -> 41466s780:RX_2 on freq 923300000 Hz at DR 8
06:05:25.299 -> 41466s846:IRQ_RX_TX_TIMEOUT
06:05:25.305 -> 41466s846:MAC rxTimeOut
06:05:25.365 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=48, Channel=13
06:20:03.353 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
06:20:03.361 -> 
06:20:03.371 -> [PIMA] Uplink routine
06:20:03.380 -> [PIMA] pima_read_cycle: start (burstMax=60)
06:20:03.387 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:20:04.809 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:06.282 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:07.753 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:09.228 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:10.646 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:11.161 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:20:11.168 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:20:11.177 -> [PIMA] pima_read_cycle: attempt 1 -> fail
06:20:11.187 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:20:12.610 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:14.081 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:15.549 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:17.020 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:18.491 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:20:18.951 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:20:18.959 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:20:19.018 -> [PIMA] pima_read_cycle: attempt 2 -> fail
06:20:19.026 -> [PIMA] pima_read_cycle: overall timeout reached
06:20:19.035 -> [PIMA] pima_read_cycle: no packet captured
06:20:19.044 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
06:20:19.054 -> 42360s653:TX on freq 917200000 Hz at DR 5
06:20:19.114 -> 42360s791:MAC txDone
06:20:24.063 -> 42365s765:RX_1 on freq 924500000 Hz at DR 13
06:20:24.120 -> 42365s806:IRQ_RX_TX_TIMEOUT
06:20:24.130 -> 42365s806:MAC rxTimeOut
06:20:25.100 -> 42366s780:RX_2 on freq 923300000 Hz at DR 8
06:20:25.156 -> 42366s846:IRQ_RX_TX_TIMEOUT
06:20:25.165 -> 42366s846:MAC rxTimeOut
06:20:25.176 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=49, Channel=10
06:35:03.186 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
06:35:03.194 -> 
06:35:03.201 -> [PIMA] Uplink routine
06:35:03.211 -> [PIMA] pima_read_cycle: start (burstMax=60)
06:35:03.220 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:35:04.643 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:06.112 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:07.583 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:09.051 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:10.521 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:10.986 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:35:10.991 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:35:11.001 -> [PIMA] pima_read_cycle: attempt 1 -> fail
06:35:11.062 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:35:12.482 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:13.957 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:15.373 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:16.846 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:18.314 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:35:18.826 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:35:18.831 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:35:18.840 -> [PIMA] pima_read_cycle: attempt 2 -> fail
06:35:18.850 -> [PIMA] pima_read_cycle: overall timeout reached
06:35:18.861 -> [PIMA] pima_read_cycle: no packet captured
06:35:18.872 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
06:35:18.882 -> 43260s653:TX on freq 917600000 Hz at DR 5
06:35:18.938 -> 43260s791:MAC txDone
06:35:23.943 -> 43265s765:RX_1 on freq 925700000 Hz at DR 13
06:35:24.001 -> 43265s806:IRQ_RX_TX_TIMEOUT
06:35:24.011 -> 43265s806:MAC rxTimeOut
06:35:24.929 -> 43266s780:RX_2 on freq 923300000 Hz at DR 8
06:35:24.987 -> 43266s846:IRQ_RX_TX_TIMEOUT
06:35:24.998 -> 43266s846:MAC rxTimeOut
06:35:25.058 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=50, Channel=12
06:50:03.058 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
06:50:03.065 -> 
06:50:03.076 -> [PIMA] Uplink routine
06:50:03.085 -> [PIMA] pima_read_cycle: start (burstMax=60)
06:50:03.095 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:50:04.515 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:05.986 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:07.408 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:08.879 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:10.350 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:10.861 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:50:10.868 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:50:10.877 -> [PIMA] pima_read_cycle: attempt 1 -> fail
06:50:10.886 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
06:50:12.309 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:13.779 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:15.248 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:16.719 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:18.193 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
06:50:18.652 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
06:50:18.657 -> [PIMA] Base frame 0x02 search timeout (no base found)
06:50:18.667 -> [PIMA] pima_read_cycle: attempt 2 -> fail
06:50:18.676 -> [PIMA] pima_read_cycle: overall timeout reached
06:50:18.686 -> [PIMA] pima_read_cycle: no packet captured
06:50:18.745 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
06:50:18.751 -> 44160s653:TX on freq 916800000 Hz at DR 5
06:50:18.813 -> 44160s791:MAC txDone
06:50:23.763 -> 44165s765:RX_1 on freq 923300000 Hz at DR 13
06:50:23.820 -> 44165s806:IRQ_RX_TX_TIMEOUT
06:50:23.828 -> 44165s806:MAC rxTimeOut
06:50:24.794 -> 44166s780:RX_2 on freq 923300000 Hz at DR 8
06:50:24.850 -> 44166s846:IRQ_RX_TX_TIMEOUT
06:50:24.858 -> 44166s846:MAC rxTimeOut
06:50:24.866 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=51, Channel=8
07:05:02.869 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
07:05:02.875 -> 
07:05:02.885 -> [PIMA] Uplink routine
07:05:02.895 -> [PIMA] pima_read_cycle: start (burstMax=60)
07:05:02.904 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:05:04.326 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:05.796 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:07.266 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:08.737 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:10.204 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:10.716 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:05:10.725 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:05:10.735 -> [PIMA] pima_read_cycle: attempt 1 -> fail
07:05:10.746 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:05:12.167 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:13.635 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:15.106 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:16.528 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:18.000 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:05:18.513 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:05:18.520 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:05:18.530 -> [PIMA] pima_read_cycle: attempt 2 -> fail
07:05:18.538 -> [PIMA] pima_read_cycle: overall timeout reached
07:05:18.549 -> [PIMA] pima_read_cycle: no packet captured
07:05:18.559 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
07:05:18.567 -> 45060s653:TX on freq 917000000 Hz at DR 5
07:05:18.626 -> 45060s791:MAC txDone
07:05:23.629 -> 45065s765:RX_1 on freq 923900000 Hz at DR 13
07:05:23.685 -> 45065s806:IRQ_RX_TX_TIMEOUT
07:05:23.691 -> 45065s806:MAC rxTimeOut
07:05:24.610 -> 45066s780:RX_2 on freq 923300000 Hz at DR 8
07:05:24.717 -> 45066s846:IRQ_RX_TX_TIMEOUT
07:05:24.724 -> 45066s846:MAC rxTimeOut
07:05:24.733 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=52, Channel=9
07:20:02.721 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
07:20:02.727 -> 
07:20:02.736 -> [PIMA] Uplink routine
07:20:02.746 -> [PIMA] pima_read_cycle: start (burstMax=60)
07:20:02.755 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:20:04.180 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:05.651 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:07.123 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:08.598 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:10.071 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:10.530 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:20:10.538 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:20:10.548 -> [PIMA] pima_read_cycle: attempt 1 -> fail
07:20:10.557 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:20:11.979 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:13.447 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:14.918 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:16.388 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:17.861 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:20:18.373 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:20:18.382 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:20:18.388 -> [PIMA] pima_read_cycle: attempt 2 -> fail
07:20:18.397 -> [PIMA] pima_read_cycle: overall timeout reached
07:20:18.407 -> [PIMA] pima_read_cycle: no packet captured
07:20:18.417 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
07:20:18.425 -> 45960s653:TX on freq 918000000 Hz at DR 5
07:20:18.488 -> 45960s791:MAC txDone
07:20:23.490 -> 45965s765:RX_1 on freq 926900000 Hz at DR 13
07:20:23.496 -> 45965s806:IRQ_RX_TX_TIMEOUT
07:20:23.507 -> 45965s806:MAC rxTimeOut
07:20:24.476 -> 45966s780:RX_2 on freq 923300000 Hz at DR 8
07:20:24.532 -> 45966s846:IRQ_RX_TX_TIMEOUT
07:20:24.538 -> 45966s846:MAC rxTimeOut
07:20:24.547 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=53, Channel=14
07:35:02.582 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
07:35:02.589 -> 
07:35:02.598 -> [PIMA] Uplink routine
07:35:02.607 -> [PIMA] pima_read_cycle: start (burstMax=60)
07:35:02.616 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:35:04.037 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:05.504 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:06.974 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:08.445 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:09.917 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:10.378 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:35:10.384 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:35:10.393 -> [PIMA] pima_read_cycle: attempt 1 -> fail
07:35:10.404 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:35:11.831 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:13.301 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:14.771 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:16.239 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:17.711 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:35:18.171 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:35:18.228 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:35:18.235 -> [PIMA] pima_read_cycle: attempt 2 -> fail
07:35:18.243 -> [PIMA] pima_read_cycle: overall timeout reached
07:35:18.251 -> [PIMA] pima_read_cycle: no packet captured
07:35:18.261 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
07:35:18.270 -> 46860s653:TX on freq 918200000 Hz at DR 5
07:35:18.326 -> 46860s791:MAC txDone
07:35:23.329 -> 46865s765:RX_1 on freq 927500000 Hz at DR 13
07:35:23.334 -> 46865s806:IRQ_RX_TX_TIMEOUT
07:35:23.343 -> 46865s806:MAC rxTimeOut
07:35:24.314 -> 46866s780:RX_2 on freq 923300000 Hz at DR 8
07:35:24.370 -> 46866s846:IRQ_RX_TX_TIMEOUT
07:35:24.377 -> 46866s846:MAC rxTimeOut
07:35:24.438 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=54, Channel=15
07:50:02.440 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
07:50:02.451 -> 
07:50:02.460 -> [PIMA] Uplink routine
07:50:02.470 -> [PIMA] pima_read_cycle: start (burstMax=60)
07:50:02.479 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:50:03.902 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:05.323 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:06.791 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:08.260 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:09.732 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:10.244 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:50:10.250 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:50:10.260 -> [PIMA] pima_read_cycle: attempt 1 -> fail
07:50:10.270 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
07:50:11.692 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:13.163 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:14.634 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:16.104 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:17.574 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
07:50:18.036 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
07:50:18.041 -> [PIMA] Base frame 0x02 search timeout (no base found)
07:50:18.051 -> [PIMA] pima_read_cycle: attempt 2 -> fail
07:50:18.061 -> [PIMA] pima_read_cycle: overall timeout reached
07:50:18.071 -> [PIMA] pima_read_cycle: no packet captured
07:50:18.131 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
07:50:18.138 -> 47760s653:TX on freq 917400000 Hz at DR 5
07:50:18.197 -> 47760s791:MAC txDone
07:50:23.142 -> 47765s765:RX_1 on freq 925100000 Hz at DR 13
07:50:23.200 -> 47765s806:IRQ_RX_TX_TIMEOUT
07:50:23.207 -> 47765s806:MAC rxTimeOut
07:50:24.176 -> 47766s780:RX_2 on freq 923300000 Hz at DR 8
07:50:24.236 -> 47766s846:IRQ_RX_TX_TIMEOUT
07:50:24.243 -> 47766s846:MAC rxTimeOut
07:50:24.252 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=55, Channel=11
08:05:02.281 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
08:05:02.287 -> 
08:05:02.296 -> [PIMA] Uplink routine
08:05:02.304 -> [PIMA] pima_read_cycle: start (burstMax=60)
08:05:02.314 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:05:03.731 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:05.202 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:06.672 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:08.143 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:09.568 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:10.080 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:05:10.087 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:05:10.095 -> [PIMA] pima_read_cycle: attempt 1 -> fail
08:05:10.104 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:05:11.527 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:12.997 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:14.462 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:15.934 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:17.402 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:05:17.866 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:05:17.871 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:05:17.928 -> [PIMA] pima_read_cycle: attempt 2 -> fail
08:05:17.935 -> [PIMA] pima_read_cycle: overall timeout reached
08:05:17.942 -> [PIMA] pima_read_cycle: no packet captured
08:05:17.951 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
08:05:17.961 -> 48660s653:TX on freq 917600000 Hz at DR 5
08:05:18.021 -> 48660s791:MAC txDone
08:05:23.024 -> 48665s765:RX_1 on freq 925700000 Hz at DR 13
08:05:23.030 -> 48665s806:IRQ_RX_TX_TIMEOUT
08:05:23.041 -> 48665s806:MAC rxTimeOut
08:05:24.010 -> 48666s780:RX_2 on freq 923300000 Hz at DR 8
08:05:24.069 -> 48666s846:IRQ_RX_TX_TIMEOUT
08:05:24.076 -> 48666s846:MAC rxTimeOut
08:05:24.087 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=56, Channel=12
08:20:02.088 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
08:20:02.095 -> 
08:20:02.105 -> [PIMA] Uplink routine
08:20:02.114 -> [PIMA] pima_read_cycle: start (burstMax=60)
08:20:02.175 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:20:03.592 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:05.014 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:06.487 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:07.958 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:09.432 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:09.942 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:20:09.952 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:20:09.960 -> [PIMA] pima_read_cycle: attempt 1 -> fail
08:20:09.969 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:20:11.389 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:12.857 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:14.329 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:15.752 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:17.226 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:20:17.737 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:20:17.742 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:20:17.752 -> [PIMA] pima_read_cycle: attempt 2 -> fail
08:20:17.758 -> [PIMA] pima_read_cycle: overall timeout reached
08:20:17.767 -> [PIMA] pima_read_cycle: no packet captured
08:20:17.773 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
08:20:17.779 -> 49560s653:TX on freq 917800000 Hz at DR 5
08:20:17.890 -> 49560s791:MAC txDone
08:20:22.839 -> 49565s765:RX_1 on freq 926300000 Hz at DR 13
08:20:22.896 -> 49565s806:IRQ_RX_TX_TIMEOUT
08:20:22.905 -> 49565s806:MAC rxTimeOut
08:20:23.873 -> 49566s780:RX_2 on freq 923300000 Hz at DR 8
08:20:23.931 -> 49566s846:IRQ_RX_TX_TIMEOUT
08:20:23.939 -> 49566s846:MAC rxTimeOut
08:20:23.951 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=57, Channel=13
08:35:01.952 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
08:35:01.958 -> 
08:35:01.967 -> [PIMA] Uplink routine
08:35:01.975 -> [PIMA] pima_read_cycle: start (burstMax=60)
08:35:01.984 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:35:03.406 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:04.878 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:06.349 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:07.822 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:09.292 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:09.753 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:35:09.760 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:35:09.769 -> [PIMA] pima_read_cycle: attempt 1 -> fail
08:35:09.775 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:35:11.246 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:12.716 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:14.138 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:15.607 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:17.077 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:35:17.592 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:35:17.602 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:35:17.612 -> [PIMA] pima_read_cycle: attempt 2 -> fail
08:35:17.623 -> [PIMA] pima_read_cycle: overall timeout reached
08:35:17.633 -> [PIMA] pima_read_cycle: no packet captured
08:35:17.643 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
08:35:17.654 -> 50460s652:TX on freq 916800000 Hz at DR 5
08:35:17.710 -> 50460s791:MAC txDone
08:35:22.708 -> 50465s764:RX_1 on freq 923300000 Hz at DR 13
08:35:22.715 -> 50465s805:IRQ_RX_TX_TIMEOUT
08:35:22.724 -> 50465s805:MAC rxTimeOut
08:35:23.693 -> 50466s779:RX_2 on freq 923300000 Hz at DR 8
08:35:23.751 -> 50466s845:IRQ_RX_TX_TIMEOUT
08:35:23.752 -> 50466s845:MAC rxTimeOut
08:35:23.813 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=58, Channel=8
08:50:01.823 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
08:50:01.827 -> 
08:50:01.838 -> [PIMA] Uplink routine
08:50:01.847 -> [PIMA] pima_read_cycle: start (burstMax=60)
08:50:01.856 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:50:03.277 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:04.749 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:06.171 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:07.641 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:09.112 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:09.624 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:50:09.634 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:50:09.643 -> [PIMA] pima_read_cycle: attempt 1 -> fail
08:50:09.652 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
08:50:11.073 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:12.542 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:14.013 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:15.485 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:16.954 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
08:50:17.412 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
08:50:17.418 -> [PIMA] Base frame 0x02 search timeout (no base found)
08:50:17.426 -> [PIMA] pima_read_cycle: attempt 2 -> fail
08:50:17.435 -> [PIMA] pima_read_cycle: overall timeout reached
08:50:17.444 -> [PIMA] pima_read_cycle: no packet captured
08:50:17.504 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
08:50:17.510 -> 51360s653:TX on freq 917000000 Hz at DR 5
08:50:17.570 -> 51360s791:MAC txDone
08:50:22.520 -> 51365s765:RX_1 on freq 923900000 Hz at DR 13
08:50:22.577 -> 51365s806:IRQ_RX_TX_TIMEOUT
08:50:22.584 -> 51365s806:MAC rxTimeOut
08:50:23.551 -> 51366s780:RX_2 on freq 923300000 Hz at DR 8
08:50:23.611 -> 51366s846:IRQ_RX_TX_TIMEOUT
08:50:23.620 -> 51366s846:MAC rxTimeOut
08:50:23.628 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=59, Channel=9
09:05:01.618 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
09:05:01.621 -> 
09:05:01.677 -> [PIMA] Uplink routine
09:05:01.681 -> [PIMA] pima_read_cycle: start (burstMax=60)
09:05:01.686 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:05:03.105 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:04.574 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:06.042 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:07.509 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:08.984 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:09.442 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:05:09.444 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:05:09.447 -> [PIMA] pima_read_cycle: attempt 1 -> fail
09:05:09.452 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:05:10.924 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:12.393 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:13.862 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:15.331 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:16.802 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:05:17.265 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:05:17.270 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:05:17.284 -> [PIMA] pima_read_cycle: attempt 2 -> fail
09:05:17.292 -> [PIMA] pima_read_cycle: overall timeout reached
09:05:17.303 -> [PIMA] pima_read_cycle: no packet captured
09:05:17.311 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
09:05:17.323 -> 52260s653:TX on freq 917200000 Hz at DR 5
09:05:17.384 -> 52260s791:MAC txDone
09:05:22.382 -> 52265s765:RX_1 on freq 924500000 Hz at DR 13
09:05:22.442 -> 52265s806:IRQ_RX_TX_TIMEOUT
09:05:22.444 -> 52265s806:MAC rxTimeOut
09:05:23.406 -> 52266s780:RX_2 on freq 923300000 Hz at DR 8
09:05:23.464 -> 52266s846:IRQ_RX_TX_TIMEOUT
09:05:23.468 -> 52266s846:MAC rxTimeOut
09:05:23.473 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=60, Channel=10
09:20:01.501 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
09:20:01.506 -> 
09:20:01.509 -> [PIMA] Uplink routine
09:20:01.518 -> [PIMA] pima_read_cycle: start (burstMax=60)
09:20:01.522 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:20:02.942 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:04.408 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:05.874 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:07.341 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:08.810 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:09.273 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:20:09.335 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:20:09.339 -> [PIMA] pima_read_cycle: attempt 1 -> fail
09:20:09.343 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:20:10.760 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:12.227 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:13.696 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:15.166 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:16.635 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:20:17.094 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:20:17.105 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:20:17.110 -> [PIMA] pima_read_cycle: attempt 2 -> fail
09:20:17.165 -> [PIMA] pima_read_cycle: overall timeout reached
09:20:17.174 -> [PIMA] pima_read_cycle: no packet captured
09:20:17.178 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
09:20:17.183 -> 53160s653:TX on freq 918000000 Hz at DR 5
09:20:17.238 -> 53160s791:MAC txDone
09:20:22.232 -> 53165s765:RX_1 on freq 926900000 Hz at DR 13
09:20:22.284 -> 53165s806:IRQ_RX_TX_TIMEOUT
09:20:22.289 -> 53165s806:MAC rxTimeOut
09:20:23.257 -> 53166s780:RX_2 on freq 923300000 Hz at DR 8
09:20:23.311 -> 53166s846:IRQ_RX_TX_TIMEOUT
09:20:23.315 -> 53166s846:MAC rxTimeOut
09:20:23.320 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=61, Channel=14
09:35:01.329 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
09:35:01.341 -> 
09:35:01.352 -> [PIMA] Uplink routine
09:35:01.380 -> [PIMA] pima_read_cycle: start (burstMax=60)
09:35:01.403 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:35:02.791 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:04.272 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:05.751 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:07.180 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:08.659 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:09.124 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:35:09.137 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:35:09.212 -> [PIMA] pima_read_cycle: attempt 1 -> fail
09:35:09.236 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:35:10.612 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:12.082 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:13.561 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:14.991 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:16.473 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:35:16.947 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:35:16.962 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:35:16.980 -> [PIMA] pima_read_cycle: attempt 2 -> fail
09:35:16.995 -> [PIMA] pima_read_cycle: overall timeout reached
09:35:17.011 -> [PIMA] pima_read_cycle: no packet captured
09:35:17.075 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
09:35:17.086 -> 54060s653:TX on freq 917400000 Hz at DR 5
09:35:17.105 -> 54060s791:MAC txDone
09:35:22.073 -> 54065s765:RX_1 on freq 925100000 Hz at DR 13
09:35:22.136 -> 54065s802:MAC rxDone
09:35:22.139 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=62, Channel=11
09:35:22.157 -> [RX] port=1 size=1
09:35:22.180 -> [RX] payload: 00 
09:35:22.188 -> [CMD] Simple command received: cmd=0x00, size=1
09:35:22.208 -> [CMD] Unknown simple command: 0x00
09:50:01.162 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
09:50:01.187 -> 
09:50:01.217 -> [PIMA] Uplink routine
09:50:01.241 -> [PIMA] pima_read_cycle: start (burstMax=60)
09:50:01.302 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:50:02.629 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:04.106 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:05.586 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:07.013 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:08.500 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:08.967 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:50:09.033 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:50:09.048 -> [PIMA] pima_read_cycle: attempt 1 -> fail
09:50:09.064 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
09:50:10.450 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:11.929 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:13.404 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:14.835 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:16.304 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
09:50:16.819 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
09:50:16.838 -> [PIMA] Base frame 0x02 search timeout (no base found)
09:50:16.846 -> [PIMA] pima_read_cycle: attempt 2 -> fail
09:50:16.857 -> [PIMA] pima_read_cycle: overall timeout reached
09:50:16.876 -> [PIMA] pima_read_cycle: no packet captured
09:50:16.892 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
09:50:16.911 -> 54960s653:TX on freq 918200000 Hz at DR 5
09:50:16.979 -> 54960s791:MAC txDone
09:50:21.942 -> 54965s765:RX_1 on freq 927500000 Hz at DR 13
09:50:21.947 -> 54965s806:IRQ_RX_TX_TIMEOUT
09:50:21.966 -> 54965s806:MAC rxTimeOut
09:50:22.943 -> 54966s780:RX_2 on freq 923300000 Hz at DR 8
09:50:23.014 -> 54966s846:IRQ_RX_TX_TIMEOUT
09:50:23.028 -> 54966s846:MAC rxTimeOut
09:50:23.043 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=63, Channel=15
10:05:01.025 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
10:05:01.032 -> 
10:05:01.037 -> [PIMA] Uplink routine
10:05:01.043 -> [PIMA] pima_read_cycle: start (burstMax=60)
10:05:01.048 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:05:02.471 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:03.937 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:05.404 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:06.870 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:08.336 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:08.844 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:05:08.849 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:05:08.854 -> [PIMA] pima_read_cycle: attempt 1 -> fail
10:05:08.860 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:05:10.278 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:11.745 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:13.212 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:14.680 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:16.146 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:05:16.655 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:05:16.660 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:05:16.665 -> [PIMA] pima_read_cycle: attempt 2 -> fail
10:05:16.670 -> [PIMA] pima_read_cycle: overall timeout reached
10:05:16.676 -> [PIMA] pima_read_cycle: no packet captured
10:05:16.682 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
10:05:16.688 -> 55860s653:TX on freq 917800000 Hz at DR 5
10:05:16.796 -> 55860s791:MAC txDone
10:05:21.747 -> 55865s765:RX_1 on freq 926300000 Hz at DR 13
10:05:21.802 -> 55865s806:IRQ_RX_TX_TIMEOUT
10:05:21.806 -> 55865s806:MAC rxTimeOut
10:05:22.769 -> 55866s780:RX_2 on freq 923300000 Hz at DR 8
10:05:22.826 -> 55866s846:IRQ_RX_TX_TIMEOUT
10:05:22.832 -> 55866s846:MAC rxTimeOut
10:05:22.839 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=64, Channel=13
10:20:00.862 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
10:20:00.867 -> 
10:20:00.871 -> [PIMA] Uplink routine
10:20:00.876 -> [PIMA] pima_read_cycle: start (burstMax=60)
10:20:00.881 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:20:02.351 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:03.818 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:05.286 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:06.705 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:08.174 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:08.682 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:20:08.689 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:20:08.694 -> [PIMA] pima_read_cycle: attempt 1 -> fail
10:20:08.699 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:20:10.170 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:11.586 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:13.051 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:14.518 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:15.985 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:20:16.497 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:20:16.502 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:20:16.510 -> [PIMA] pima_read_cycle: attempt 2 -> fail
10:20:16.517 -> [PIMA] pima_read_cycle: overall timeout reached
10:20:16.522 -> [PIMA] pima_read_cycle: no packet captured
10:20:16.527 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
10:20:16.532 -> 56760s653:TX on freq 917000000 Hz at DR 5
10:20:16.636 -> 56760s791:MAC txDone
10:20:21.589 -> 56765s765:RX_1 on freq 923900000 Hz at DR 13
10:20:21.648 -> 56765s806:IRQ_RX_TX_TIMEOUT
10:20:21.650 -> 56765s806:MAC rxTimeOut
10:20:22.611 -> 56766s780:RX_2 on freq 923300000 Hz at DR 8
10:20:22.671 -> 56766s846:IRQ_RX_TX_TIMEOUT
10:20:22.674 -> 56766s846:MAC rxTimeOut
10:20:22.676 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=65, Channel=9
10:35:00.706 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
10:35:00.713 -> 
10:35:00.721 -> [PIMA] Uplink routine
10:35:00.724 -> [PIMA] pima_read_cycle: start (burstMax=60)
10:35:00.727 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:35:02.195 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:03.664 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:05.131 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:06.550 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:08.016 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:08.533 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:35:08.539 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:35:08.543 -> [PIMA] pima_read_cycle: attempt 1 -> fail
10:35:08.545 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:35:10.013 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:11.482 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:12.907 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:14.375 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:15.847 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:35:16.357 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:35:16.361 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:35:16.367 -> [PIMA] pima_read_cycle: attempt 2 -> fail
10:35:16.372 -> [PIMA] pima_read_cycle: overall timeout reached
10:35:16.377 -> [PIMA] pima_read_cycle: no packet captured
10:35:16.381 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
10:35:16.383 -> 57660s652:TX on freq 917400000 Hz at DR 5
10:35:16.488 -> 57660s791:MAC txDone
10:35:21.441 -> 57665s764:RX_1 on freq 925100000 Hz at DR 13
10:35:21.497 -> 57665s805:MAC rxDone
10:35:21.502 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=66, Channel=11
10:35:21.506 -> [RX] port=1 size=1
10:35:21.513 -> [RX] payload: 00 
10:35:21.519 -> [CMD] Simple command received: cmd=0x00, size=1
10:35:21.524 -> [CMD] Unknown simple command: 0x00
10:50:00.585 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
10:50:00.592 -> 
10:50:00.602 -> [PIMA] Uplink routine
10:50:00.612 -> [PIMA] pima_read_cycle: start (burstMax=60)
10:50:00.620 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:50:02.037 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:03.501 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:04.971 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:06.445 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:07.861 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:08.369 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:50:08.373 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:50:08.379 -> [PIMA] pima_read_cycle: attempt 1 -> fail
10:50:08.385 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
10:50:09.852 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:11.318 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:12.785 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:14.252 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:15.678 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
10:50:16.189 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
10:50:16.203 -> [PIMA] Base frame 0x02 search timeout (no base found)
10:50:16.212 -> [PIMA] pima_read_cycle: attempt 2 -> fail
10:50:16.218 -> [PIMA] pima_read_cycle: overall timeout reached
10:50:16.225 -> [PIMA] pima_read_cycle: no packet captured
10:50:16.232 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
10:50:16.237 -> 58560s653:TX on freq 916800000 Hz at DR 5
10:50:16.343 -> 58560s791:MAC txDone
10:50:21.286 -> 58565s765:RX_1 on freq 923300000 Hz at DR 13
10:50:21.342 -> 58565s804:MAC rxDone
10:50:21.349 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=67, Channel=8
10:50:21.355 -> [RX] port=0 size=0
11:05:00.411 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
11:05:00.415 -> 
11:05:00.419 -> [PIMA] Uplink routine
11:05:00.423 -> [PIMA] pima_read_cycle: start (burstMax=60)
11:05:00.429 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:05:01.853 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:03.321 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:04.798 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:06.271 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:07.739 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:08.198 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:05:08.251 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:05:08.255 -> [PIMA] pima_read_cycle: attempt 1 -> fail
11:05:08.260 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:05:09.676 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:11.141 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:12.609 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:14.076 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:15.542 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:05:16.052 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:05:16.055 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:05:16.060 -> [PIMA] pima_read_cycle: attempt 2 -> fail
11:05:16.063 -> [PIMA] pima_read_cycle: overall timeout reached
11:05:16.066 -> [PIMA] pima_read_cycle: no packet captured
11:05:16.071 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
11:05:16.077 -> 59460s653:TX on freq 917200000 Hz at DR 5
11:05:16.184 -> 59460s791:MAC txDone
11:05:21.144 -> 59465s765:RX_1 on freq 924500000 Hz at DR 13
11:05:21.196 -> 59465s806:IRQ_RX_TX_TIMEOUT
11:05:21.205 -> 59465s806:MAC rxTimeOut
11:05:22.173 -> 59466s780:RX_2 on freq 923300000 Hz at DR 8
11:05:22.227 -> 59466s846:IRQ_RX_TX_TIMEOUT
11:05:22.231 -> 59466s846:MAC rxTimeOut
11:05:22.235 -> 59466s852:TX on freq 918200000 Hz at DR 5
11:05:22.392 -> 59466s989:MAC txDone
11:05:27.338 -> 59471s962:RX_1 on freq 927500000 Hz at DR 13
11:05:27.392 -> 59472s003:IRQ_RX_TX_TIMEOUT
11:05:27.397 -> 59472s003:MAC rxTimeOut
11:05:28.361 -> 59472s977:RX_2 on freq 923300000 Hz at DR 8
11:05:28.419 -> 59473s043:IRQ_RX_TX_TIMEOUT
11:05:28.429 -> 59473s043:MAC rxTimeOut
11:05:28.436 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=68, Channel=15
11:20:00.260 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
11:20:00.265 -> 
11:20:00.270 -> [PIMA] Uplink routine
11:20:00.273 -> [PIMA] pima_read_cycle: start (burstMax=60)
11:20:00.277 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:20:01.743 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:03.161 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:04.625 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:06.094 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:07.561 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:08.069 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:20:08.071 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:20:08.074 -> [PIMA] pima_read_cycle: attempt 1 -> fail
11:20:08.077 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:20:09.546 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:11.011 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:12.479 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:13.945 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:15.410 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:20:15.869 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:20:15.871 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:20:15.875 -> [PIMA] pima_read_cycle: attempt 2 -> fail
11:20:15.879 -> [PIMA] pima_read_cycle: overall timeout reached
11:20:15.935 -> [PIMA] pima_read_cycle: no packet captured
11:20:15.938 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
11:20:15.943 -> 60360s653:TX on freq 917600000 Hz at DR 5
11:20:15.999 -> 60360s791:MAC txDone
11:20:21.004 -> 60365s765:RX_1 on freq 925700000 Hz at DR 13
11:20:21.057 -> 60365s806:IRQ_RX_TX_TIMEOUT
11:20:21.062 -> 60365s806:MAC rxTimeOut
11:20:22.028 -> 60366s780:RX_2 on freq 923300000 Hz at DR 8
11:20:22.084 -> 60366s845:IRQ_RX_TX_TIMEOUT
11:20:22.086 -> 60366s846:MAC rxTimeOut
11:20:22.089 -> 60366s852:TX on freq 918000000 Hz at DR 5
11:20:22.193 -> 60366s989:MAC txDone
11:20:27.196 -> 60371s962:RX_1 on freq 926900000 Hz at DR 13
11:20:27.252 -> 60372s003:IRQ_RX_TX_TIMEOUT
11:20:27.256 -> 60372s003:MAC rxTimeOut
11:20:28.219 -> 60372s977:RX_2 on freq 923300000 Hz at DR 8
11:20:28.274 -> 60373s043:IRQ_RX_TX_TIMEOUT
11:20:28.277 -> 60373s043:MAC rxTimeOut
11:20:28.282 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=69, Channel=14
11:35:00.107 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
11:35:00.112 -> 
11:35:00.117 -> [PIMA] Uplink routine
11:35:00.120 -> [PIMA] pima_read_cycle: start (burstMax=60)
11:35:00.123 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:35:01.590 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:03.055 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:04.520 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:05.937 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:07.404 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:07.916 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:35:07.919 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:35:07.924 -> [PIMA] pima_read_cycle: attempt 1 -> fail
11:35:07.928 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:35:09.398 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:10.864 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:12.330 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:13.751 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:15.218 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:35:15.730 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:35:15.737 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:35:15.742 -> [PIMA] pima_read_cycle: attempt 2 -> fail
11:35:15.747 -> [PIMA] pima_read_cycle: overall timeout reached
11:35:15.751 -> [PIMA] pima_read_cycle: no packet captured
11:35:15.756 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
11:35:15.758 -> 61260s653:TX on freq 917800000 Hz at DR 5
11:35:15.864 -> 61260s791:MAC txDone
11:35:20.860 -> 61265s765:RX_1 on freq 926300000 Hz at DR 13
11:35:20.864 -> 61265s806:IRQ_RX_TX_TIMEOUT
11:35:20.867 -> 61265s806:MAC rxTimeOut
11:35:21.878 -> 61266s780:RX_2 on freq 923300000 Hz at DR 8
11:35:21.941 -> 61266s845:IRQ_RX_TX_TIMEOUT
11:35:21.947 -> 61266s846:MAC rxTimeOut
11:35:21.956 -> 61266s852:TX on freq 917400000 Hz at DR 5
11:35:22.068 -> 61266s989:MAC txDone
11:35:27.018 -> 61271s962:RX_1 on freq 925100000 Hz at DR 13
11:35:27.074 -> 61272s002:MAC rxDone
11:35:27.077 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=70, Channel=11
11:35:27.080 -> [RX] port=0 size=0
11:49:59.948 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
11:49:59.950 -> 
11:49:59.954 -> [PIMA] Uplink routine
11:49:59.957 -> [PIMA] pima_read_cycle: start (burstMax=60)
11:49:59.964 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:50:01.432 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:02.898 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:04.364 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:05.832 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:07.252 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:07.766 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:50:07.767 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:50:07.770 -> [PIMA] pima_read_cycle: attempt 1 -> fail
11:50:07.773 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
11:50:09.238 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:10.708 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:12.176 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:13.594 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:15.059 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
11:50:15.571 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
11:50:15.572 -> [PIMA] Base frame 0x02 search timeout (no base found)
11:50:15.575 -> [PIMA] pima_read_cycle: attempt 2 -> fail
11:50:15.581 -> [PIMA] pima_read_cycle: overall timeout reached
11:50:15.587 -> [PIMA] pima_read_cycle: no packet captured
11:50:15.590 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
11:50:15.646 -> 62160s653:TX on freq 917200000 Hz at DR 5
11:50:15.702 -> 62160s791:MAC txDone
11:50:20.698 -> 62165s765:RX_1 on freq 924500000 Hz at DR 13
11:50:20.753 -> 62165s805:MAC rxDone
11:50:20.756 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=71, Channel=10
11:50:20.759 -> [RX] port=0 size=0
12:04:59.803 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
12:04:59.806 -> 
12:04:59.813 -> [PIMA] Uplink routine
12:04:59.818 -> [PIMA] pima_read_cycle: start (burstMax=60)
12:04:59.824 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:05:01.244 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:02.712 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:04.182 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:05.649 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:07.115 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:07.621 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:05:07.626 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:05:07.629 -> [PIMA] pima_read_cycle: attempt 1 -> fail
12:05:07.634 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:05:09.051 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:10.520 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:11.985 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:13.450 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:14.924 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:05:15.431 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:05:15.437 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:05:15.441 -> [PIMA] pima_read_cycle: attempt 2 -> fail
12:05:15.446 -> [PIMA] pima_read_cycle: overall timeout reached
12:05:15.451 -> [PIMA] pima_read_cycle: no packet captured
12:05:15.459 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
12:05:15.466 -> 63060s653:TX on freq 918000000 Hz at DR 5
12:05:15.574 -> 63060s791:MAC txDone
12:05:20.522 -> 63065s765:RX_1 on freq 926900000 Hz at DR 13
12:05:20.578 -> 63065s806:IRQ_RX_TX_TIMEOUT
12:05:20.581 -> 63065s806:MAC rxTimeOut
12:05:21.545 -> 63066s780:RX_2 on freq 923300000 Hz at DR 8
12:05:21.598 -> 63066s845:IRQ_RX_TX_TIMEOUT
12:05:21.600 -> 63066s846:MAC rxTimeOut
12:05:21.602 -> 63066s852:TX on freq 917000000 Hz at DR 5
12:05:21.757 -> 63066s989:MAC txDone
12:05:26.710 -> 63071s962:RX_1 on freq 923900000 Hz at DR 13
12:05:26.765 -> 63072s002:MAC rxDone
12:05:26.769 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=72, Channel=9
12:05:26.776 -> [RX] port=0 size=0
12:19:59.666 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
12:19:59.670 -> 
12:19:59.674 -> [PIMA] Uplink routine
12:19:59.679 -> [PIMA] pima_read_cycle: start (burstMax=60)
12:19:59.684 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:20:01.101 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:02.567 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:04.036 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:05.510 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:06.978 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:07.436 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:20:07.445 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:20:07.504 -> [PIMA] pima_read_cycle: attempt 1 -> fail
12:20:07.513 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:20:08.934 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:10.402 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:11.871 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:13.292 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:14.761 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:20:15.268 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:20:15.277 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:20:15.283 -> [PIMA] pima_read_cycle: attempt 2 -> fail
12:20:15.288 -> [PIMA] pima_read_cycle: overall timeout reached
12:20:15.293 -> [PIMA] pima_read_cycle: no packet captured
12:20:15.297 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
12:20:15.302 -> 63960s652:TX on freq 917600000 Hz at DR 5
12:20:15.409 -> 63960s791:MAC txDone
12:20:20.361 -> 63965s764:RX_1 on freq 925700000 Hz at DR 13
12:20:20.420 -> 63965s805:IRQ_RX_TX_TIMEOUT
12:20:20.430 -> 63965s805:MAC rxTimeOut
12:20:21.400 -> 63966s779:RX_2 on freq 923300000 Hz at DR 8
12:20:21.459 -> 63966s844:IRQ_RX_TX_TIMEOUT
12:20:21.463 -> 63966s845:MAC rxTimeOut
12:20:21.468 -> 63966s851:TX on freq 916800000 Hz at DR 5
12:20:21.623 -> 63966s988:MAC txDone
12:20:26.576 -> 63971s961:RX_1 on freq 923300000 Hz at DR 13
12:20:26.630 -> 63972s002:IRQ_RX_TX_TIMEOUT
12:20:26.634 -> 63972s002:MAC rxTimeOut
12:20:27.606 -> 63972s976:RX_2 on freq 923300000 Hz at DR 8
12:20:27.662 -> 63973s041:IRQ_RX_TX_TIMEOUT
12:20:27.667 -> 63973s042:MAC rxTimeOut
12:20:27.672 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=73, Channel=8
12:34:59.511 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
12:34:59.512 -> 
12:34:59.517 -> [PIMA] Uplink routine
12:34:59.520 -> [PIMA] pima_read_cycle: start (burstMax=60)
12:34:59.523 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:35:00.938 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:02.405 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:03.877 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:05.349 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:06.818 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:07.278 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:35:07.335 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:35:07.345 -> [PIMA] pima_read_cycle: attempt 1 -> fail
12:35:07.354 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:35:08.777 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:10.246 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:11.721 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:13.139 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:14.607 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:35:15.122 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:35:15.127 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:35:15.130 -> [PIMA] pima_read_cycle: attempt 2 -> fail
12:35:15.135 -> [PIMA] pima_read_cycle: overall timeout reached
12:35:15.140 -> [PIMA] pima_read_cycle: no packet captured
12:35:15.144 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
12:35:15.148 -> 64860s653:TX on freq 918200000 Hz at DR 5
12:35:15.254 -> 64860s791:MAC txDone
12:35:20.213 -> 64865s765:RX_1 on freq 927500000 Hz at DR 13
12:35:20.266 -> 64865s806:IRQ_RX_TX_TIMEOUT
12:35:20.268 -> 64865s806:MAC rxTimeOut
12:35:21.233 -> 64866s780:RX_2 on freq 923300000 Hz at DR 8
12:35:21.288 -> 64866s845:IRQ_RX_TX_TIMEOUT
12:35:21.343 -> 64866s846:MAC rxTimeOut
12:35:21.346 -> 64866s852:TX on freq 917800000 Hz at DR 5
12:35:21.452 -> 64866s989:MAC txDone
12:35:26.408 -> 64871s962:RX_1 on freq 926300000 Hz at DR 13
12:35:26.463 -> 64872s003:IRQ_RX_TX_TIMEOUT
12:35:26.467 -> 64872s003:MAC rxTimeOut
12:35:27.431 -> 64872s977:RX_2 on freq 923300000 Hz at DR 8
12:35:27.485 -> 64873s042:IRQ_RX_TX_TIMEOUT
12:35:27.487 -> 64873s043:MAC rxTimeOut
12:35:27.541 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=74, Channel=13
12:49:59.358 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
12:49:59.363 -> 
12:49:59.369 -> [PIMA] Uplink routine
12:49:59.374 -> [PIMA] pima_read_cycle: start (burstMax=60)
12:49:59.381 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:50:00.800 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:02.271 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:03.741 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:05.208 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:06.686 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:07.145 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:50:07.151 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:50:07.160 -> [PIMA] pima_read_cycle: attempt 1 -> fail
12:50:07.165 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
12:50:08.637 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:10.060 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:11.527 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:13.005 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:14.472 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
12:50:14.982 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
12:50:14.986 -> [PIMA] Base frame 0x02 search timeout (no base found)
12:50:14.991 -> [PIMA] pima_read_cycle: attempt 2 -> fail
12:50:14.996 -> [PIMA] pima_read_cycle: overall timeout reached
12:50:15.000 -> [PIMA] pima_read_cycle: no packet captured
12:50:15.006 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
12:50:15.009 -> 65760s653:TX on freq 917600000 Hz at DR 5
12:50:15.114 -> 65760s791:MAC txDone
12:50:20.069 -> 65765s765:RX_1 on freq 925700000 Hz at DR 13
12:50:20.125 -> 65765s806:IRQ_RX_TX_TIMEOUT
12:50:20.131 -> 65765s806:MAC rxTimeOut
12:50:21.094 -> 65766s780:RX_2 on freq 923300000 Hz at DR 8
12:50:21.150 -> 65766s845:IRQ_RX_TX_TIMEOUT
12:50:21.158 -> 65766s846:MAC rxTimeOut
12:50:21.166 -> 65766s852:TX on freq 918000000 Hz at DR 5
12:50:21.275 -> 65766s989:MAC txDone
12:50:26.281 -> 65771s962:RX_1 on freq 926900000 Hz at DR 13
12:50:26.341 -> 65772s003:IRQ_RX_TX_TIMEOUT
12:50:26.349 -> 65772s003:MAC rxTimeOut
12:50:27.314 -> 65772s977:RX_2 on freq 923300000 Hz at DR 8
12:50:27.372 -> 65773s042:IRQ_RX_TX_TIMEOUT
12:50:27.381 -> 65773s043:MAC rxTimeOut
12:50:27.390 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=75, Channel=14
13:04:59.181 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
13:04:59.192 -> 
13:04:59.199 -> [PIMA] Uplink routine
13:04:59.209 -> [PIMA] pima_read_cycle: start (burstMax=60)
13:04:59.214 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:05:00.635 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:02.101 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:03.570 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:05.038 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:06.510 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:07.022 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:05:07.029 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:05:07.034 -> [PIMA] pima_read_cycle: attempt 1 -> fail
13:05:07.038 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:05:08.456 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:09.933 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:11.403 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:12.874 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:14.346 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:05:14.804 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:05:14.811 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:05:14.817 -> [PIMA] pima_read_cycle: attempt 2 -> fail
13:05:14.823 -> [PIMA] pima_read_cycle: overall timeout reached
13:05:14.827 -> [PIMA] pima_read_cycle: no packet captured
13:05:14.882 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
13:05:14.885 -> 66660s652:TX on freq 917200000 Hz at DR 5
13:05:14.941 -> 66660s791:MAC txDone
13:05:19.946 -> 66665s764:RX_1 on freq 924500000 Hz at DR 13
13:05:19.955 -> 66665s805:IRQ_RX_TX_TIMEOUT
13:05:19.958 -> 66665s805:MAC rxTimeOut
13:05:20.922 -> 66666s779:RX_2 on freq 923300000 Hz at DR 8
13:05:21.028 -> 66666s844:IRQ_RX_TX_TIMEOUT
13:05:21.035 -> 66666s845:MAC rxTimeOut
13:05:21.042 -> 66666s851:TX on freq 917000000 Hz at DR 5
13:05:21.150 -> 66666s988:MAC txDone
13:05:26.099 -> 66671s961:RX_1 on freq 923900000 Hz at DR 13
13:05:26.158 -> 66672s002:IRQ_RX_TX_TIMEOUT
13:05:26.164 -> 66672s002:MAC rxTimeOut
13:05:27.130 -> 66672s976:RX_2 on freq 923300000 Hz at DR 8
13:05:27.188 -> 66673s041:IRQ_RX_TX_TIMEOUT
13:05:27.193 -> 66673s042:MAC rxTimeOut
13:05:27.199 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=76, Channel=9
13:19:59.055 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
13:19:59.065 -> 
13:19:59.070 -> [PIMA] Uplink routine
13:19:59.074 -> [PIMA] pima_read_cycle: start (burstMax=60)
13:19:59.076 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:20:00.494 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:01.965 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:03.439 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:04.914 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:06.334 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:06.847 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:20:06.850 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:20:06.858 -> [PIMA] pima_read_cycle: attempt 1 -> fail
13:20:06.865 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:20:08.335 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:09.751 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:11.219 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:12.687 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:14.155 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:20:14.665 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:20:14.675 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:20:14.684 -> [PIMA] pima_read_cycle: attempt 2 -> fail
13:20:14.692 -> [PIMA] pima_read_cycle: overall timeout reached
13:20:14.696 -> [PIMA] pima_read_cycle: no packet captured
13:20:14.701 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
13:20:14.707 -> 67560s653:TX on freq 916800000 Hz at DR 5
13:20:14.813 -> 67560s791:MAC txDone
13:20:19.763 -> 67565s765:RX_1 on freq 923300000 Hz at DR 13
13:20:19.823 -> 67565s806:IRQ_RX_TX_TIMEOUT
13:20:19.830 -> 67565s806:MAC rxTimeOut
13:20:20.801 -> 67566s780:RX_2 on freq 923300000 Hz at DR 8
13:20:20.859 -> 67566s845:IRQ_RX_TX_TIMEOUT
13:20:20.867 -> 67566s846:MAC rxTimeOut
13:20:20.873 -> 67566s852:TX on freq 918200000 Hz at DR 5
13:20:20.980 -> 67566s989:MAC txDone
13:20:25.988 -> 67571s962:RX_1 on freq 927500000 Hz at DR 13
13:20:25.990 -> 67572s001:MAC rxDone
13:20:25.994 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=77, Channel=15
13:20:26.050 -> [RX] port=0 size=0
13:34:58.902 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
13:34:58.906 -> 
13:34:58.912 -> [PIMA] Uplink routine
13:34:58.918 -> [PIMA] pima_read_cycle: start (burstMax=60)
13:34:58.925 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:35:00.345 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:01.814 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:03.282 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:04.752 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:06.219 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:06.685 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:35:06.691 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:35:06.695 -> [PIMA] pima_read_cycle: attempt 1 -> fail
13:35:06.701 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:35:08.171 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:09.637 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:11.105 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:12.573 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:13.999 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:35:14.510 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:35:14.519 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:35:14.527 -> [PIMA] pima_read_cycle: attempt 2 -> fail
13:35:14.536 -> [PIMA] pima_read_cycle: overall timeout reached
13:35:14.541 -> [PIMA] pima_read_cycle: no packet captured
13:35:14.546 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
13:35:14.552 -> 68460s653:TX on freq 917400000 Hz at DR 5
13:35:14.659 -> 68460s791:MAC txDone
13:35:19.616 -> 68465s765:RX_1 on freq 925100000 Hz at DR 13
13:35:19.672 -> 68465s806:IRQ_RX_TX_TIMEOUT
13:35:19.674 -> 68465s806:MAC rxTimeOut
13:35:20.636 -> 68466s780:RX_2 on freq 923300000 Hz at DR 8
13:35:20.689 -> 68466s845:IRQ_RX_TX_TIMEOUT
13:35:20.693 -> 68466s846:MAC rxTimeOut
13:35:20.697 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=78, Channel=11
13:49:58.735 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
13:49:58.742 -> 
13:49:58.750 -> [PIMA] Uplink routine
13:49:58.754 -> [PIMA] pima_read_cycle: start (burstMax=60)
13:49:58.759 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:50:00.178 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:01.643 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:03.113 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:04.580 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:06.048 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:06.564 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:50:06.569 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:50:06.575 -> [PIMA] pima_read_cycle: attempt 1 -> fail
13:50:06.580 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
13:50:08.000 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:09.472 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:10.946 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:12.414 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:13.885 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
13:50:14.342 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
13:50:14.346 -> [PIMA] Base frame 0x02 search timeout (no base found)
13:50:14.355 -> [PIMA] pima_read_cycle: attempt 2 -> fail
13:50:14.412 -> [PIMA] pima_read_cycle: overall timeout reached
13:50:14.418 -> [PIMA] pima_read_cycle: no packet captured
13:50:14.424 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
13:50:14.428 -> 69360s653:TX on freq 917800000 Hz at DR 5
13:50:14.485 -> 69360s791:MAC txDone
13:50:19.491 -> 69365s765:RX_1 on freq 926300000 Hz at DR 13
13:50:19.496 -> 69365s806:IRQ_RX_TX_TIMEOUT
13:50:19.503 -> 69365s806:MAC rxTimeOut
13:50:20.470 -> 69366s780:RX_2 on freq 923300000 Hz at DR 8
13:50:20.525 -> 69366s845:IRQ_RX_TX_TIMEOUT
13:50:20.580 -> 69366s846:MAC rxTimeOut
13:50:20.590 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=79, Channel=13
14:04:58.583 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
14:04:58.594 -> 
14:04:58.600 -> [PIMA] Uplink routine
14:04:58.608 -> [PIMA] pima_read_cycle: start (burstMax=60)
14:04:58.611 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:05:00.030 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:01.498 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:02.968 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:04.439 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:05.906 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:06.369 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:05:06.421 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:05:06.424 -> [PIMA] pima_read_cycle: attempt 1 -> fail
14:05:06.427 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:05:07.842 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:09.316 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:10.785 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:12.252 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:13.721 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:05:14.178 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:05:14.233 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:05:14.240 -> [PIMA] pima_read_cycle: attempt 2 -> fail
14:05:14.249 -> [PIMA] pima_read_cycle: overall timeout reached
14:05:14.258 -> [PIMA] pima_read_cycle: no packet captured
14:05:14.265 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
14:05:14.269 -> 70260s653:TX on freq 917400000 Hz at DR 5
14:05:14.325 -> 70260s791:MAC txDone
14:05:19.327 -> 70265s765:RX_1 on freq 925100000 Hz at DR 13
14:05:19.382 -> 70265s806:IRQ_RX_TX_TIMEOUT
14:05:19.386 -> 70265s806:MAC rxTimeOut
14:05:20.352 -> 70266s780:RX_2 on freq 923300000 Hz at DR 8
14:05:20.410 -> 70266s845:IRQ_RX_TX_TIMEOUT
14:05:20.414 -> 70266s846:MAC rxTimeOut
14:05:20.419 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=80, Channel=11
14:19:58.434 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
14:19:58.438 -> 
14:19:58.444 -> [PIMA] Uplink routine
14:19:58.449 -> [PIMA] pima_read_cycle: start (burstMax=60)
14:19:58.453 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:19:59.875 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:01.344 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:02.811 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:04.281 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:05.753 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:06.217 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:20:06.272 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:20:06.277 -> [PIMA] pima_read_cycle: attempt 1 -> fail
14:20:06.281 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:20:07.699 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:09.165 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:10.634 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:12.102 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:13.570 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:20:14.028 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:20:14.084 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:20:14.087 -> [PIMA] pima_read_cycle: attempt 2 -> fail
14:20:14.092 -> [PIMA] pima_read_cycle: overall timeout reached
14:20:14.097 -> [PIMA] pima_read_cycle: no packet captured
14:20:14.102 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
14:20:14.108 -> 71160s653:TX on freq 918000000 Hz at DR 5
14:20:14.215 -> 71160s791:MAC txDone
14:20:19.171 -> 71165s765:RX_1 on freq 926900000 Hz at DR 13
14:20:19.230 -> 71165s806:IRQ_RX_TX_TIMEOUT
14:20:19.240 -> 71165s806:MAC rxTimeOut
14:20:20.205 -> 71166s780:RX_2 on freq 923300000 Hz at DR 8
14:20:20.266 -> 71166s845:IRQ_RX_TX_TIMEOUT
14:20:20.272 -> 71166s846:MAC rxTimeOut
14:20:20.275 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=81, Channel=14
14:34:58.288 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
14:34:58.298 -> 
14:34:58.304 -> [PIMA] Uplink routine
14:34:58.306 -> [PIMA] pima_read_cycle: start (burstMax=60)
14:34:58.312 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:34:59.732 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:01.203 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:02.678 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:04.145 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:05.612 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:06.075 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:35:06.081 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:35:06.086 -> [PIMA] pima_read_cycle: attempt 1 -> fail
14:35:06.144 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:35:07.564 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:09.037 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:10.505 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:11.974 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:13.391 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:35:13.903 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:35:13.912 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:35:13.922 -> [PIMA] pima_read_cycle: attempt 2 -> fail
14:35:13.934 -> [PIMA] pima_read_cycle: overall timeout reached
14:35:13.940 -> [PIMA] pima_read_cycle: no packet captured
14:35:13.944 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
14:35:13.951 -> 72060s653:TX on freq 917200000 Hz at DR 5
14:35:14.057 -> 72060s791:MAC txDone
14:35:19.005 -> 72065s765:RX_1 on freq 924500000 Hz at DR 13
14:35:19.061 -> 72065s806:IRQ_RX_TX_TIMEOUT
14:35:19.065 -> 72065s806:MAC rxTimeOut
14:35:20.031 -> 72066s780:RX_2 on freq 923300000 Hz at DR 8
14:35:20.091 -> 72066s845:IRQ_RX_TX_TIMEOUT
14:35:20.094 -> 72066s846:MAC rxTimeOut
14:35:20.098 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=82, Channel=10
14:49:58.144 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
14:49:58.147 -> 
14:49:58.152 -> [PIMA] Uplink routine
14:49:58.155 -> [PIMA] pima_read_cycle: start (burstMax=60)
14:49:58.158 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:49:59.575 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:01.046 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:02.513 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:03.982 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:05.447 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:05.955 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:50:05.964 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:50:05.975 -> [PIMA] pima_read_cycle: attempt 1 -> fail
14:50:05.983 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
14:50:07.403 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:08.870 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:10.341 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:11.809 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:13.278 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
14:50:13.740 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
14:50:13.750 -> [PIMA] Base frame 0x02 search timeout (no base found)
14:50:13.753 -> [PIMA] pima_read_cycle: attempt 2 -> fail
14:50:13.756 -> [PIMA] pima_read_cycle: overall timeout reached
14:50:13.810 -> [PIMA] pima_read_cycle: no packet captured
14:50:13.814 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
14:50:13.819 -> 72960s653:TX on freq 917000000 Hz at DR 5
14:50:13.874 -> 72960s791:MAC txDone
14:50:18.875 -> 72965s765:RX_1 on freq 923900000 Hz at DR 13
14:50:18.930 -> 72965s806:IRQ_RX_TX_TIMEOUT
14:50:18.937 -> 72965s806:MAC rxTimeOut
14:50:19.905 -> 72966s780:RX_2 on freq 923300000 Hz at DR 8
14:50:19.959 -> 72966s845:IRQ_RX_TX_TIMEOUT
14:50:19.962 -> 72966s846:MAC rxTimeOut
14:50:19.968 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=83, Channel=9
15:04:58.003 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
15:04:58.009 -> 
15:04:58.013 -> [PIMA] Uplink routine
15:04:58.019 -> [PIMA] pima_read_cycle: start (burstMax=60)
15:04:58.023 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:04:59.440 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:00.907 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:02.382 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:03.849 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:05.316 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:05.779 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:05:05.787 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:05:05.797 -> [PIMA] pima_read_cycle: attempt 1 -> fail
15:05:05.805 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:05:07.274 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:08.694 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:10.163 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:11.637 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:13.107 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:05:13.619 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:05:13.629 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:05:13.638 -> [PIMA] pima_read_cycle: attempt 2 -> fail
15:05:13.648 -> [PIMA] pima_read_cycle: overall timeout reached
15:05:13.655 -> [PIMA] pima_read_cycle: no packet captured
15:05:13.660 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
15:05:13.666 -> 73860s653:TX on freq 917600000 Hz at DR 5
15:05:13.719 -> 73860s791:MAC txDone
15:05:18.722 -> 73865s765:RX_1 on freq 925700000 Hz at DR 13
15:05:18.778 -> 73865s806:IRQ_RX_TX_TIMEOUT
15:05:18.781 -> 73865s806:MAC rxTimeOut
15:05:19.748 -> 73866s780:RX_2 on freq 923300000 Hz at DR 8
15:05:19.802 -> 73866s845:IRQ_RX_TX_TIMEOUT
15:05:19.806 -> 73866s846:MAC rxTimeOut
15:05:19.810 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=84, Channel=12
15:19:57.837 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
15:19:57.843 -> 
15:19:57.849 -> [PIMA] Uplink routine
15:19:57.854 -> [PIMA] pima_read_cycle: start (burstMax=60)
15:19:57.856 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:19:59.277 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:00.746 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:02.213 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:03.681 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:05.152 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:05.619 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:20:05.672 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:20:05.683 -> [PIMA] pima_read_cycle: attempt 1 -> fail
15:20:05.693 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:20:07.114 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:08.589 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:10.009 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:11.477 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:12.950 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:20:13.459 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:20:13.462 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:20:13.465 -> [PIMA] pima_read_cycle: attempt 2 -> fail
15:20:13.471 -> [PIMA] pima_read_cycle: overall timeout reached
15:20:13.475 -> [PIMA] pima_read_cycle: no packet captured
15:20:13.480 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
15:20:13.486 -> 74760s653:TX on freq 916800000 Hz at DR 5
15:20:13.591 -> 74760s791:MAC txDone
15:20:18.547 -> 74765s765:RX_1 on freq 923300000 Hz at DR 13
15:20:18.605 -> 74765s806:IRQ_RX_TX_TIMEOUT
15:20:18.611 -> 74765s806:MAC rxTimeOut
15:20:19.574 -> 74766s780:RX_2 on freq 923300000 Hz at DR 8
15:20:19.634 -> 74766s845:IRQ_RX_TX_TIMEOUT
15:20:19.641 -> 74766s846:MAC rxTimeOut
15:20:19.646 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=85, Channel=8
15:34:57.658 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
15:34:57.669 -> 
15:34:57.675 -> [PIMA] Uplink routine
15:34:57.681 -> [PIMA] pima_read_cycle: start (burstMax=60)
15:34:57.737 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:34:59.159 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:00.626 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:02.048 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:03.518 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:04.986 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:05.502 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:35:05.506 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:35:05.511 -> [PIMA] pima_read_cycle: attempt 1 -> fail
15:35:05.517 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:35:06.933 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:08.403 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:09.877 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:11.341 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:12.808 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:35:13.316 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:35:13.323 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:35:13.333 -> [PIMA] pima_read_cycle: attempt 2 -> fail
15:35:13.342 -> [PIMA] pima_read_cycle: overall timeout reached
15:35:13.346 -> [PIMA] pima_read_cycle: no packet captured
15:35:13.351 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
15:35:13.356 -> 75660s653:TX on freq 918200000 Hz at DR 5
15:35:13.462 -> 75660s791:MAC txDone
15:35:18.419 -> 75665s765:RX_1 on freq 927500000 Hz at DR 13
15:35:18.477 -> 75665s806:IRQ_RX_TX_TIMEOUT
15:35:18.485 -> 75665s806:MAC rxTimeOut
15:35:19.448 -> 75666s780:RX_2 on freq 923300000 Hz at DR 8
15:35:19.505 -> 75666s845:IRQ_RX_TX_TIMEOUT
15:35:19.510 -> 75666s846:MAC rxTimeOut
15:35:19.512 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=86, Channel=15
15:49:57.527 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
15:49:57.535 -> 
15:49:57.541 -> [PIMA] Uplink routine
15:49:57.549 -> [PIMA] pima_read_cycle: start (burstMax=60)
15:49:57.555 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:49:58.974 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:00.442 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:01.913 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:03.381 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:04.849 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:05.314 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:50:05.369 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:50:05.376 -> [PIMA] pima_read_cycle: attempt 1 -> fail
15:50:05.384 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
15:50:06.802 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:08.277 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:09.749 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:11.219 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:12.642 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
15:50:13.151 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
15:50:13.160 -> [PIMA] Base frame 0x02 search timeout (no base found)
15:50:13.165 -> [PIMA] pima_read_cycle: attempt 2 -> fail
15:50:13.171 -> [PIMA] pima_read_cycle: overall timeout reached
15:50:13.176 -> [PIMA] pima_read_cycle: no packet captured
15:50:13.180 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
15:50:13.183 -> 76560s653:TX on freq 917800000 Hz at DR 5
15:50:13.288 -> 76560s791:MAC txDone
15:50:18.240 -> 76565s765:RX_1 on freq 926300000 Hz at DR 13
15:50:18.296 -> 76565s806:IRQ_RX_TX_TIMEOUT
15:50:18.302 -> 76565s806:MAC rxTimeOut
15:50:19.266 -> 76566s780:RX_2 on freq 923300000 Hz at DR 8
15:50:19.322 -> 76566s845:IRQ_RX_TX_TIMEOUT
15:50:19.328 -> 76566s846:MAC rxTimeOut
15:50:19.388 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=87, Channel=13
16:04:57.372 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
16:04:57.376 -> 
16:04:57.381 -> [PIMA] Uplink routine
16:04:57.384 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:04:57.387 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:04:58.854 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:00.326 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:01.745 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:03.216 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:04.686 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:05.194 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:05:05.196 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:05:05.200 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:05:05.206 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:05:06.626 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:08.097 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:09.571 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:11.040 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:12.509 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:05:12.975 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:05:13.029 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:05:13.034 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:05:13.039 -> [PIMA] pima_read_cycle: overall timeout reached
16:05:13.047 -> [PIMA] pima_read_cycle: no packet captured
16:05:13.051 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:05:13.055 -> 77460s653:TX on freq 916800000 Hz at DR 5
16:05:13.160 -> 77460s791:MAC txDone
16:05:18.116 -> 77465s765:RX_1 on freq 923300000 Hz at DR 13
16:05:18.169 -> 77465s806:IRQ_RX_TX_TIMEOUT
16:05:18.175 -> 77465s806:MAC rxTimeOut
16:05:19.139 -> 77466s780:RX_2 on freq 923300000 Hz at DR 8
16:05:19.194 -> 77466s845:IRQ_RX_TX_TIMEOUT
16:05:19.200 -> 77466s846:MAC rxTimeOut
16:05:19.205 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=88, Channel=8
16:19:57.237 -> [LORA] Next period armed: 900000 ms (phaseOnce=2037)
16:19:57.244 -> 
16:19:57.251 -> [PIMA] Uplink routine
16:19:57.256 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:19:57.261 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:19:58.680 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:00.148 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:01.621 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:03.095 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:04.567 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:05.033 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:20:05.037 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:20:05.042 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:20:05.046 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:20:06.517 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:07.941 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:09.409 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:10.879 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:12.351 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:20:12.862 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:20:12.869 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:20:12.876 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:20:12.882 -> [PIMA] pima_read_cycle: overall timeout reached
16:20:12.888 -> [PIMA] pima_read_cycle: no packet captured
16:20:12.892 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:20:12.895 -> 78360s652:TX on freq 917600000 Hz at DR 5
16:20:13.003 -> 78360s791:MAC txDone
16:20:17.953 -> 78365s764:RX_1 on freq 925700000 Hz at DR 13
16:20:18.011 -> 78365s805:IRQ_RX_TX_TIMEOUT
16:20:18.015 -> 78365s805:MAC rxTimeOut
16:20:18.978 -> 78366s779:RX_2 on freq 923300000 Hz at DR 8
16:20:19.033 -> 78366s844:IRQ_RX_TX_TIMEOUT
16:20:19.039 -> 78366s845:MAC rxTimeOut
16:20:19.044 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=89, Channel=12
16:34:18.005 -> [KEYS] Loaded from flash
16:34:18.060 -> DEVEUI:ac1f0926002f0003
16:34:18.063 -> APPKEY:f2839693c180a9df89412e3098ba5a43
16:34:18.064 -> MODEL:ST-EAM-01B
16:34:18.065 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
16:34:18.068 -> 5s052:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
16:34:18.078 -> [LORA] Starting join (OTAA)
16:34:18.081 -> 5s059:TX on freq 915600000 Hz at DR 2
16:34:18.436 -> 5s432:MAC txDone
16:34:23.381 -> 10s409:RX_1 on freq 924500000 Hz at DR 10
16:34:23.434 -> 10s458:IRQ_RX_TX_TIMEOUT
16:34:23.439 -> 10s458:MAC rxTimeOut
16:34:24.404 -> 11s420:RX_2 on freq 923300000 Hz at DR 8
16:34:24.463 -> 11s486:IRQ_RX_TX_TIMEOUT
16:34:24.466 -> 11s487:MAC rxTimeOut
16:34:24.467 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
16:34:24.489 -> 
16:34:24.490 -> [LORA] JOIN FAILED (status=-1) count=1
16:34:24.513 -> [LORA] Rejoin scheduled
16:34:34.457 -> 21s493:TX on freq 917600000 Hz at DR 2
16:34:34.459 -> [LORA] Rejoin busy -> retry in 5000 ms
16:34:34.825 -> 21s866:MAC txDone
16:34:39.473 -> [LORA] Rejoin busy -> retry in 5000 ms
16:34:39.834 -> 26s843:RX_1 on freq 925700000 Hz at DR 10
16:34:39.947 -> 26s982:MAC rxDone
16:34:39.959 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
16:34:40.027 -> 27s003:RX_C on freq 923300000 Hz at DR 8
16:34:40.037 -> [LORA] Switch to Class C done
16:34:40.049 -> 
16:34:40.066 -> [LORA] JOINED (OTAA)
16:34:40.084 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
16:34:40.103 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
16:34:40.113 -> ###### NwkSKey:     06:B8:17:89:BE:07:3D:3D:0C:12:F8:26:B5:C3:33:2A
16:34:40.124 -> ###### AppSKey:     FF:91:9D:28:31:61:B3:FB:BA:D2:02:94:CC:00:64:7F
16:34:47.962 -> [PIMA] B1 warmup uplink
16:34:47.976 -> 
16:34:47.995 -> [PIMA] Uplink routine
16:34:48.015 -> [BOOT] Sending initial warmup byte (B1)
16:34:48.086 -> 35s004:TX on freq 916800000 Hz at DR 2
16:34:48.293 -> 35s295:MAC txDone
16:34:48.307 -> 35s296:RX_C on freq 923300000 Hz at DR 8
16:34:53.225 -> 40s266:RX_1 on freq 923300000 Hz at DR 10
16:34:53.336 -> 40s380:MAC rxDone
16:34:53.404 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=8
16:34:53.408 -> [RX] port=0 size=0
16:34:53.424 -> 40s387:RX_C on freq 923300000 Hz at DR 8
16:34:55.970 -> [PIMA] First read after boot
16:34:55.990 -> [PIMA] Changing to OTAA_PERIOD mode
16:34:55.997 -> [LORA] Phase offset applied once: 3244 ms (base=900000 ms)
16:34:56.020 -> 
16:34:56.050 -> [PIMA] Uplink routine
16:34:56.069 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:34:56.134 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:34:57.470 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:34:58.895 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:00.375 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:01.858 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:03.282 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:03.800 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:35:03.818 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:35:03.847 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:35:03.870 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:35:05.254 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:06.737 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:08.162 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:09.633 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:11.112 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:35:11.579 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:35:11.637 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:35:11.651 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:35:11.675 -> [PIMA] pima_read_cycle: overall timeout reached
16:35:11.698 -> [PIMA] pima_read_cycle: no packet captured
16:35:11.719 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:35:11.731 -> 58s629:TX on freq 917200000 Hz at DR 5
16:35:11.801 -> 58s773:MAC txDone
16:35:11.807 -> 58s774:RX_C on freq 923300000 Hz at DR 8
16:35:16.712 -> 63s741:RX_1 on freq 924500000 Hz at DR 13
16:35:16.765 -> 63s787:MAC rxDone
16:35:16.776 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=10
16:35:16.799 -> [RX] port=0 size=0
16:35:16.812 -> 63s794:RX_C on freq 923300000 Hz at DR 8
16:36:45.755 -> 152s814:MAC rxDone
16:36:45.768 -> 152s820:RX_C on freq 923300000 Hz at DR 8
16:36:50.436 -> 157s461:MAC rxDone
16:36:50.457 -> 157s468:RX_C on freq 923300000 Hz at DR 8
16:39:30.845 -> [KEYS] Loaded from flash
16:39:30.900 -> DEVEUI:ac1f0926002f0003
16:39:30.904 -> APPKEY:f2839693c180a9df89412e3098ba5a43
16:39:30.908 -> MODEL:ST-EAM-01B
16:39:30.913 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
16:39:30.917 -> 5s052:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
16:39:30.933 -> [LORA] Starting join (OTAA)
16:39:30.939 -> 5s059:TX on freq 915200000 Hz at DR 2
16:39:31.246 -> 5s432:MAC txDone
16:39:36.249 -> 10s409:RX_1 on freq 923300000 Hz at DR 10
16:39:36.306 -> 10s458:IRQ_RX_TX_TIMEOUT
16:39:36.308 -> 10s458:MAC rxTimeOut
16:39:37.273 -> 11s420:RX_2 on freq 923300000 Hz at DR 8
16:39:37.327 -> 11s486:IRQ_RX_TX_TIMEOUT
16:39:37.329 -> 11s487:MAC rxTimeOut
16:39:37.336 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
16:39:37.341 -> 
16:39:37.346 -> [LORA] JOIN FAILED (status=-1) count=1
16:39:37.352 -> [LORA] Rejoin scheduled
16:39:47.298 -> 21s493:TX on freq 917000000 Hz at DR 2
16:39:47.300 -> [LORA] Rejoin busy -> retry in 5000 ms
16:39:47.707 -> 21s866:MAC txDone
16:39:52.303 -> [LORA] Rejoin busy -> retry in 5000 ms
16:39:52.662 -> 26s843:RX_1 on freq 923900000 Hz at DR 10
16:39:52.818 -> 26s982:MAC rxDone
16:39:52.819 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
16:39:52.821 -> 27s003:RX_C on freq 923300000 Hz at DR 8
16:39:52.824 -> [LORA] Switch to Class C done
16:39:52.826 -> 
16:39:52.829 -> [LORA] JOINED (OTAA)
16:39:52.833 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
16:39:52.886 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
16:39:52.887 -> ###### NwkSKey:     E9:C4:A7:EC:38:BD:E0:90:09:3D:02:47:31:A4:83:32
16:39:52.891 -> ###### AppSKey:     AA:7D:50:B9:8B:A7:69:D6:EB:B4:71:2F:40:6F:09:5C
16:40:00.816 -> [PIMA] B1 warmup uplink
16:40:00.819 -> 
16:40:00.827 -> [PIMA] Uplink routine
16:40:00.832 -> [BOOT] Sending initial warmup byte (B1)
16:40:00.835 -> 35s004:TX on freq 918200000 Hz at DR 2
16:40:01.140 -> 35s295:MAC txDone
16:40:01.142 -> 35s296:RX_C on freq 923300000 Hz at DR 8
16:40:06.094 -> 40s266:RX_1 on freq 927500000 Hz at DR 10
16:40:06.200 -> 40s380:MAC rxDone
16:40:06.207 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=15
16:40:06.213 -> [RX] port=0 size=0
16:40:06.220 -> 40s388:RX_C on freq 923300000 Hz at DR 8
16:40:08.798 -> [PIMA] First read after boot
16:40:08.856 -> [PIMA] Changing to OTAA_PERIOD mode
16:40:08.862 -> [LORA] Phase offset applied once: 3244 ms (base=900000 ms)
16:40:08.871 -> 
16:40:08.881 -> [PIMA] Uplink routine
16:40:08.889 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:40:08.900 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:40:10.268 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:11.738 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:13.208 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:14.676 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:16.141 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:16.654 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:40:16.661 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:40:16.668 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:40:16.675 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:40:18.095 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:19.561 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:21.030 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:22.502 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:23.973 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:40:24.436 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:40:24.441 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:40:24.446 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:40:24.501 -> [PIMA] pima_read_cycle: overall timeout reached
16:40:24.508 -> [PIMA] pima_read_cycle: no packet captured
16:40:24.514 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:40:24.519 -> 58s629:TX on freq 917400000 Hz at DR 5
16:40:24.576 -> 58s778:MAC txDone
16:40:24.585 -> 58s779:RX_C on freq 923300000 Hz at DR 8
16:40:28.830 -> 62s995:MAC rxDone
16:40:28.832 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=11
16:40:28.835 -> 63s001:RX_C on freq 923300000 Hz at DR 8
16:40:29.547 -> 63s747:RX_1 on freq 925100000 Hz at DR 13
16:40:29.601 -> 63s792:MAC rxDone
16:40:29.603 -> [RX] port=0 size=0
16:40:29.609 -> 63s799:RX_C on freq 923300000 Hz at DR 8
16:41:05.955 -> 100s131:MAC rxDone
16:41:05.962 -> 100s137:RX_C on freq 923300000 Hz at DR 8
16:43:03.432 -> 217s639:MAC rxDone
16:43:03.451 -> [RX] port=1 size=1
16:43:03.478 -> [RX] payload: 04 
16:43:03.499 -> [CMD] Simple command received: cmd=0x04, size=1
16:43:03.527 -> [CMD] Reboot requested
16:43:03.549 -> [CMD] ACK cmd=0x04 status=OK
16:43:03.572 -> [CMD] SendResponse: size=1
16:43:03.595 -> 217s647:TX on freq 916800000 Hz at DR 5
16:43:03.613 -> [CMD] Rebooting in 300 ms...
16:43:03.688 -> 217s701:MAC txDone
16:43:03.751 -> [BOOT] APP V1.2.0
16:43:03.754 -> [BOOT] LoRaWAN MW V2.4.0
16:43:03.779 -> [BOOT] Radio PHY V1.2.0
16:43:03.793 -> [LORA] NVM data restored
16:43:03.816 -> ###### IDs  ######
16:43:03.826 -> ###### DevEui:      AC:1F:09:26:00:2F:00:03
16:43:03.890 -> 
16:43:03.908 -> ###### AppEui:      00:00:00:00:00:00:00:00
16:43:03.936 -> ###### DevAddr:     05:6C:52:23
16:43:03.961 -> [LORA] AU915 sub-band 2 applied
16:43:03.989 -> [HP] Loaded from flash: DISABLED (raw=0)
16:43:04.015 -> [OTAA] Period loaded from flash: 900000 ms
16:43:04.033 -> [HP] High Precision Mode: DISABLED (fromFlash=1)
16:43:04.053 -> [OTAA] Base period at boot: 900000 ms (fromFlash=1)
16:43:04.073 -> [BOOT] Waiting 5 seconds before JOIN...
16:43:08.788 -> [KEYS] Loaded from flash
16:43:08.804 -> DEVEUI:ac1f0926002f0003
16:43:08.820 -> APPKEY:f2839693c180a9df89412e3098ba5a43
16:43:08.837 -> MODEL:ST-EAM-01B
16:43:08.905 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
16:43:08.912 -> 5s051:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
16:43:08.954 -> [LORA] Starting join (OTAA)
16:43:08.969 -> 5s058:TX on freq 915600000 Hz at DR 2
16:43:09.174 -> 5s431:MAC txDone
16:43:14.135 -> 10s408:RX_1 on freq 924500000 Hz at DR 10
16:43:14.190 -> 10s458:IRQ_RX_TX_TIMEOUT
16:43:14.207 -> 10s458:MAC rxTimeOut
16:43:15.184 -> 11s419:RX_2 on freq 923300000 Hz at DR 8
16:43:15.237 -> 11s485:IRQ_RX_TX_TIMEOUT
16:43:15.247 -> 11s486:MAC rxTimeOut
16:43:15.258 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
16:43:15.281 -> 
16:43:15.299 -> [LORA] JOIN FAILED (status=-1) count=1
16:43:15.317 -> [LORA] Rejoin scheduled
16:43:25.221 -> 21s492:TX on freq 917400000 Hz at DR 2
16:43:25.233 -> [LORA] Rejoin busy -> retry in 5000 ms
16:43:25.595 -> 21s865:MAC txDone
16:43:30.256 -> [LORA] Rejoin busy -> retry in 5000 ms
16:43:30.570 -> 26s842:RX_1 on freq 925100000 Hz at DR 10
16:43:30.736 -> 26s981:MAC rxDone
16:43:30.747 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
16:43:30.770 -> 
16:43:30.789 -> [LORA] JOINED (OTAA)
16:43:30.813 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
16:43:30.832 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
16:43:30.849 -> ###### NwkSKey:     5C:B0:54:B9:D4:01:72:4F:41:CF:7A:18:82:EB:1F:16
16:43:30.870 -> ###### AppSKey:     EE:8D:FA:47:66:77:E8:07:48:69:1F:1D:3B:50:B6:60
16:43:38.713 -> [PIMA] B1 warmup uplink
16:43:38.732 -> 
16:43:38.741 -> [PIMA] Uplink routine
16:43:38.770 -> [BOOT] Sending initial warmup byte (B1)
16:43:38.787 -> 34s991:TX on freq 917600000 Hz at DR 2
16:43:39.001 -> 35s283:MAC txDone
16:43:44.015 -> 40s259:RX_1 on freq 925700000 Hz at DR 10
16:43:44.124 -> 40s368:MAC rxDone
16:43:44.137 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=12
16:43:44.157 -> [RX] port=0 size=0
16:43:46.705 -> [PIMA] First read after boot
16:43:46.725 -> [PIMA] Changing to OTAA_PERIOD mode
16:43:46.792 -> [LORA] Phase offset applied once: 2037 ms (base=900000 ms)
16:43:46.805 -> 
16:43:46.817 -> [PIMA] Uplink routine
16:43:46.841 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:43:46.851 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:43:48.185 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:43:49.666 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:43:51.138 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:43:52.566 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:43:54.040 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:43:54.561 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:43:54.573 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:43:54.584 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:43:54.597 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:43:56.022 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:43:57.448 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:43:58.919 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:44:00.397 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:44:01.863 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:44:02.336 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:44:02.351 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:44:02.362 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:44:02.431 -> [PIMA] pima_read_cycle: overall timeout reached
16:44:02.449 -> [PIMA] pima_read_cycle: no packet captured
16:44:02.462 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:44:02.482 -> 58s616:TX on freq 917000000 Hz at DR 5
16:44:02.550 -> 58s760:MAC txDone
16:44:07.448 -> 63s734:RX_1 on freq 923900000 Hz at DR 13
16:44:07.512 -> 63s774:MAC rxDone
16:44:07.523 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=9
16:44:07.544 -> [RX] port=0 size=0
16:47:28.802 -> [KEYS] Loaded from flash
16:47:28.855 -> DEVEUI:ac1f0926002f0003
16:47:28.855 -> APPKEY:f2839693c180a9df89412e3098ba5a43
16:47:28.858 -> MODEL:ST-EAM-01B
16:47:28.862 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
16:47:28.863 -> 5s052:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
16:47:28.871 -> [LORA] Starting join (OTAA)
16:47:28.873 -> 5s059:TX on freq 916000000 Hz at DR 2
16:47:29.228 -> 5s432:MAC txDone
16:47:34.225 -> 10s409:RX_1 on freq 925700000 Hz at DR 10
16:47:34.279 -> 10s458:IRQ_RX_TX_TIMEOUT
16:47:34.282 -> 10s458:MAC rxTimeOut
16:47:35.194 -> 11s420:RX_2 on freq 923300000 Hz at DR 8
16:47:35.299 -> 11s487:IRQ_RX_TX_TIMEOUT
16:47:35.303 -> 11s487:MAC rxTimeOut
16:47:35.310 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
16:47:35.315 -> 
16:47:35.322 -> [LORA] JOIN FAILED (status=-1) count=1
16:47:35.326 -> [LORA] Rejoin scheduled
16:47:45.271 -> 21s493:TX on freq 917800000 Hz at DR 2
16:47:45.273 -> [LORA] Rejoin busy -> retry in 5000 ms
16:47:45.638 -> 21s866:MAC txDone
16:47:50.284 -> [LORA] Rejoin busy -> retry in 5000 ms
16:47:50.642 -> 26s843:RX_1 on freq 926300000 Hz at DR 10
16:47:50.756 -> 26s982:MAC rxDone
16:47:50.763 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
16:47:50.826 -> 27s003:RX_C on freq 923300000 Hz at DR 8
16:47:50.835 -> [LORA] Switch to Class C done
16:47:50.848 -> 
16:47:50.862 -> [LORA] JOINED (OTAA)
16:47:50.875 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
16:47:50.890 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
16:47:50.906 -> ###### NwkSKey:     4C:DE:C4:F8:E9:AB:72:AE:EE:04:80:34:ED:C9:6F:B1
16:47:50.922 -> ###### AppSKey:     C1:D7:CA:C5:A1:83:F2:F3:1B:13:C1:ED:C8:45:B2:0C
16:47:58.802 -> [PIMA] B1 warmup uplink
16:47:58.813 -> 
16:47:58.831 -> [PIMA] Uplink routine
16:47:58.840 -> [BOOT] Sending initial warmup byte (B1)
16:47:58.851 -> 35s004:TX on freq 917400000 Hz at DR 2
16:47:59.061 -> 35s295:MAC txDone
16:47:59.124 -> 35s296:RX_C on freq 923300000 Hz at DR 8
16:48:04.080 -> 40s266:RX_1 on freq 925100000 Hz at DR 10
16:48:04.148 -> 40s380:MAC rxDone
16:48:04.207 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=11
16:48:04.220 -> [RX] port=0 size=0
16:48:04.242 -> 40s387:RX_C on freq 923300000 Hz at DR 8
16:48:06.784 -> [PIMA] First read after boot
16:48:06.796 -> [PIMA] Changing to OTAA_PERIOD mode
16:48:06.818 -> [LORA] Phase offset applied once: 3244 ms (base=900000 ms)
16:48:06.832 -> 
16:48:06.851 -> [PIMA] Uplink routine
16:48:06.863 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:48:06.925 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:48:08.254 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:09.731 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:11.210 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:12.635 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:14.109 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:14.592 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:48:14.598 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:48:14.644 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:48:14.741 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:48:16.062 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:17.535 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:19.013 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:20.483 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:21.909 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:48:22.436 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:48:22.443 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:48:22.460 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:48:22.477 -> [PIMA] pima_read_cycle: overall timeout reached
16:48:22.497 -> [PIMA] pima_read_cycle: no packet captured
16:48:22.508 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:48:22.528 -> 58s629:TX on freq 917200000 Hz at DR 5
16:48:22.599 -> 58s773:MAC txDone
16:48:22.606 -> 58s774:RX_C on freq 923300000 Hz at DR 8
16:48:27.518 -> 63s741:RX_1 on freq 924500000 Hz at DR 13
16:48:27.581 -> 63s787:MAC rxDone
16:48:27.582 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=10
16:48:27.596 -> [RX] port=0 size=0
16:48:27.605 -> 63s794:RX_C on freq 923300000 Hz at DR 8
16:49:26.409 -> 122s657:MAC rxDone
16:49:26.477 -> 122s663:RX_C on freq 923300000 Hz at DR 8
16:51:43.421 -> [KEYS] Loaded from flash
16:51:43.426 -> DEVEUI:ac1f0926002f0003
16:51:43.431 -> APPKEY:f2839693c180a9df89412e3098ba5a43
16:51:43.435 -> MODEL:ST-EAM-01B
16:51:43.490 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
16:51:43.496 -> 5s052:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
16:51:43.514 -> [LORA] Starting join (OTAA)
16:51:43.519 -> 5s059:TX on freq 915800000 Hz at DR 2
16:51:43.829 -> 5s432:MAC txDone
16:51:48.772 -> 10s409:RX_1 on freq 925100000 Hz at DR 10
16:51:48.825 -> 10s458:IRQ_RX_TX_TIMEOUT
16:51:48.830 -> 10s458:MAC rxTimeOut
16:51:49.798 -> 11s420:RX_2 on freq 923300000 Hz at DR 8
16:51:49.855 -> 11s486:IRQ_RX_TX_TIMEOUT
16:51:49.860 -> 11s487:MAC rxTimeOut
16:51:49.871 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
16:51:49.879 -> 
16:51:49.887 -> [LORA] JOIN FAILED (status=-1) count=1
16:51:49.950 -> [LORA] Rejoin scheduled
16:51:59.897 -> 21s493:TX on freq 917400000 Hz at DR 2
16:51:59.908 -> [LORA] Rejoin busy -> retry in 5000 ms
16:52:00.224 -> 21s866:MAC txDone
16:52:04.873 -> [LORA] Rejoin busy -> retry in 5000 ms
16:52:05.233 -> 26s843:RX_1 on freq 925100000 Hz at DR 10
16:52:05.346 -> 26s982:MAC rxDone
16:52:05.354 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
16:52:05.423 -> 27s003:RX_C on freq 923300000 Hz at DR 8
16:52:05.426 -> [LORA] Switch to Class C done
16:52:05.443 -> 
16:52:05.460 -> [LORA] JOINED (OTAA)
16:52:05.473 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
16:52:05.491 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
16:52:05.501 -> ###### NwkSKey:     17:F5:7C:2B:FF:91:6A:C2:96:DB:1D:92:3C:B1:70:70
16:52:05.519 -> ###### AppSKey:     97:7F:DA:CD:6D:44:1B:F6:9B:7D:47:E8:C4:1B:97:87
16:52:13.404 -> [PIMA] B1 warmup uplink
16:52:13.412 -> 
16:52:13.433 -> [PIMA] Uplink routine
16:52:13.452 -> [BOOT] Sending initial warmup byte (B1)
16:52:13.469 -> 35s004:TX on freq 917600000 Hz at DR 2
16:52:13.690 -> 35s295:MAC txDone
16:52:13.701 -> 35s296:RX_C on freq 923300000 Hz at DR 8
16:52:18.669 -> 40s266:RX_1 on freq 925700000 Hz at DR 10
16:52:18.740 -> 40s380:MAC rxDone
16:52:18.753 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=12
16:52:18.774 -> [RX] port=0 size=0
16:52:18.848 -> 40s387:RX_C on freq 923300000 Hz at DR 8
16:52:21.386 -> [PIMA] First read after boot
16:52:21.395 -> [PIMA] Changing to OTAA_PERIOD mode
16:52:21.406 -> [LORA] Phase offset applied once: 3244 ms (base=900000 ms)
16:52:21.426 -> 
16:52:21.449 -> [PIMA] Uplink routine
16:52:21.459 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:52:21.484 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:52:22.861 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:24.289 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:25.756 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:27.233 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:28.706 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:29.176 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:52:29.189 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:52:29.214 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:52:29.276 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:52:30.660 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:32.136 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:33.607 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:35.072 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:36.499 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:52:37.019 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:52:37.038 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:52:37.064 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:52:37.083 -> [PIMA] pima_read_cycle: overall timeout reached
16:52:37.103 -> [PIMA] pima_read_cycle: no packet captured
16:52:37.125 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:52:37.147 -> 58s629:TX on freq 917200000 Hz at DR 5
16:52:37.212 -> 58s773:MAC txDone
16:52:37.226 -> 58s774:RX_C on freq 923300000 Hz at DR 8
16:52:42.092 -> 63s741:RX_1 on freq 924500000 Hz at DR 13
16:52:42.164 -> 63s787:MAC rxDone
16:52:42.178 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=10
16:52:42.199 -> [RX] port=0 size=0
16:52:42.223 -> 63s794:RX_C on freq 923300000 Hz at DR 8
16:53:14.393 -> 96s031:MAC rxDone
16:53:14.403 -> 96s037:RX_C on freq 923300000 Hz at DR 8
16:53:14.668 -> 96s325:MAC rxDone
16:53:14.731 -> 96s331:RX_C on freq 923300000 Hz at DR 8
16:55:06.103 -> 207s756:MAC rxDone
16:55:06.115 -> [RX] port=1 size=1
16:55:06.128 -> [RX] payload: 04 
16:55:06.153 -> [CMD] Simple command received: cmd=0x04, size=1
16:55:06.169 -> [CMD] Reboot requested
16:55:06.195 -> [CMD] ACK cmd=0x04 status=OK
16:55:06.213 -> [CMD] SendResponse: size=1
16:55:06.236 -> 207s764:TX on freq 916800000 Hz at DR 5
16:55:06.303 -> [CMD] Rebooting in 300 ms...
16:55:06.306 -> 207s818:MAC txDone
16:55:06.434 -> [BOOT] APP V1.2.0
16:55:06.450 -> [BOOT] LoRaWAN MW V2.4.0
16:55:06.474 -> [BOOT] Radio PHY V1.2.0
16:55:06.503 -> [LORA] NVM data restored
16:55:06.515 -> ###### IDs  ######
16:55:06.529 -> ###### DevEui:      AC:1F:09:26:00:2F:00:03
16:55:06.541 -> ###### AppEui:      00:00:00:00:00:00:00:00
16:55:06.562 -> ###### DevAddr:     05:6C:52:23
16:55:06.625 -> [LORA] AU915 sub-band 2 applied
16:55:06.635 -> [HP] Loaded from flash: DISABLED (raw=0)
16:55:06.657 -> [OTAA] Period loaded from flash: 900000 ms
16:55:06.678 -> [HP] High Precision Mode: DISABLED (fromFlash=1)
16:55:06.700 -> [OTAA] Base period at boot: 900000 ms (fromFlash=1)
16:55:06.711 -> [BOOT] Waiting 5 seconds before JOIN...
16:55:11.469 -> [KEYS] Loaded from flash
16:55:11.476 -> DEVEUI:ac1f0926002f0003
16:55:11.487 -> APPKEY:f2839693c180a9df89412e3098ba5a43
16:55:11.495 -> MODEL:ST-EAM-01B
16:55:11.505 -> [SEAIOT_LABEL] {"deveui":"ac1f0926002f0003","appkey":"f2839693c180a9df89412e3098ba5a43","model":"ST-EAM-01B"}
16:55:11.564 -> 5s051:[LORA] JoinEUI override -> equal to DevEUI: AC:1F:09:26:00:2F:00:03
16:55:11.578 -> [LORA] Starting join (OTAA)
16:55:11.583 -> 5s058:TX on freq 916000000 Hz at DR 2
16:55:11.841 -> 5s431:MAC txDone
16:55:16.840 -> 10s408:RX_1 on freq 925700000 Hz at DR 10
16:55:16.896 -> 10s458:IRQ_RX_TX_TIMEOUT
16:55:16.903 -> 10s458:MAC rxTimeOut
16:55:17.815 -> 11s419:RX_2 on freq 923300000 Hz at DR 8
16:55:17.923 -> 11s485:IRQ_RX_TX_TIMEOUT
16:55:17.928 -> 11s486:MAC rxTimeOut
16:55:17.938 -> [LORA] OnTxData: status=4, DR=0, UplinkCounter=0, Channel=0
16:55:17.944 -> 
16:55:17.953 -> [LORA] JOIN FAILED (status=-1) count=1
16:55:17.954 -> [LORA] Rejoin scheduled
16:55:27.897 -> 21s492:TX on freq 917000000 Hz at DR 2
16:55:27.915 -> [LORA] Rejoin busy -> retry in 5000 ms
16:55:28.290 -> 21s865:MAC txDone
16:55:32.903 -> [LORA] Rejoin busy -> retry in 5000 ms
16:55:33.265 -> 26s842:RX_1 on freq 923900000 Hz at DR 10
16:55:33.385 -> 26s981:MAC rxDone
16:55:33.393 -> [LORA] OnTxData: status=0, DR=0, UplinkCounter=0, Channel=0
16:55:33.408 -> 
16:55:33.424 -> [LORA] JOINED (OTAA)
16:55:33.491 -> ###### MCRootKey:   6E:29:EF:3A:7B:13:83:06:BB:DC:36:38:38:BA:D3:FA
16:55:33.502 -> ###### MCKEKey:     61:FB:EF:02:F0:F9:1E:A4:C4:21:D7:9F:1C:9D:F2:0D
16:55:33.510 -> ###### NwkSKey:     30:3B:A8:90:18:1B:55:00:A8:A0:7F:C3:F1:59:E6:3A
16:55:33.536 -> ###### AppSKey:     3D:79:13:0E:54:2D:9B:5E:5C:F7:88:E3:70:83:E6:8A
16:55:41.382 -> [PIMA] B1 warmup uplink
16:55:41.395 -> 
16:55:41.409 -> [PIMA] Uplink routine
16:55:41.478 -> [BOOT] Sending initial warmup byte (B1)
16:55:41.489 -> 34s991:TX on freq 918200000 Hz at DR 2
16:55:41.712 -> 35s283:MAC txDone
16:55:46.667 -> 40s259:RX_1 on freq 927500000 Hz at DR 10
16:55:46.775 -> 40s368:MAC rxDone
16:55:46.780 -> [LORA] OnTxData: status=0, DR=2, UplinkCounter=1, Channel=15
16:55:46.812 -> [RX] port=0 size=0
16:55:49.414 -> [PIMA] First read after boot
16:55:49.422 -> [PIMA] Changing to OTAA_PERIOD mode
16:55:49.444 -> [LORA] Phase offset applied once: 2037 ms (base=900000 ms)
16:55:49.467 -> 
16:55:49.492 -> [PIMA] Uplink routine
16:55:49.500 -> [PIMA] pima_read_cycle: start (burstMax=60)
16:55:49.523 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:55:50.850 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:55:52.323 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:55:53.796 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:55:55.269 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:55:56.745 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:55:57.212 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:55:57.223 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:55:57.244 -> [PIMA] pima_read_cycle: attempt 1 -> fail
16:55:57.263 -> [PIMA] pima_read_base_frame: start (timeout=8000 ms)
16:55:58.697 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:56:00.118 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:56:01.595 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:56:03.081 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:56:04.556 -> [PIMA] pima_read_frame_any: timeout (search=1500 ms)
16:56:05.021 -> [PIMA] pima_read_frame_any: timeout (search=500 ms)
16:56:05.034 -> [PIMA] Base frame 0x02 search timeout (no base found)
16:56:05.056 -> [PIMA] pima_read_cycle: attempt 2 -> fail
16:56:05.079 -> [PIMA] pima_read_cycle: overall timeout reached
16:56:05.099 -> [PIMA] pima_read_cycle: no packet captured
16:56:05.122 -> [PIMA] Read failed (ok=0, len=0) -> sending FF burst
16:56:05.184 -> 58s617:TX on freq 917800000 Hz at DR 5
16:56:05.198 -> 58s760:MAC txDone
16:56:10.158 -> 63s734:RX_1 on freq 926300000 Hz at DR 13
16:56:10.172 -> 63s774:MAC rxDone
16:56:10.236 -> [LORA] OnTxData: status=0, DR=5, UplinkCounter=2, Channel=13
16:56:10.251 -> [RX] port=0 size=0
